HWiNFO64 Version 7.20-4700

HYDEV-ASTER ---------------------------------------------------------------

 [Current Computer]
  Computer Name:                          HYDEV-ASTER
  Computer Brand Name:                    Acidanthera iMacPro1,1
 [Operating System]
  Operating System:                       Microsoft Windows 11 Professional (x64) Build 22000.739
  UEFI Boot:                              Present
  Secure Boot:                            Disabled
  Hypervisor-protected Code Integrity (HVCI): Disabled
  Virtual Machine Warning:                Microsoft Hyper-V is active. Some results may not reflect real hardware !

Central Processor(s) ------------------------------------------------------

 [CPU Unit Count]
  Number Of Processor Packages (Physical): 1
  Number Of Processor Cores:              18
  Number Of Logical Processors:           36

Intel Xeon E5-2696 v3 -----------------------------------------------------

 [General Information]
  Processor Name:                         Intel Xeon E5-2696 v3
  Original Processor Frequency:           2300.0 MHz
  Original Processor Frequency [MHz]:     2300
  CPU ID:                                 000306F2
  CPU Brand Name:                         Intel(R) Xeon(R) CPU E5-2696 v3 @ 2.30GHz
  CPU Vendor:                             GenuineIntel
  CPU Stepping:                           C0/C1
  CPU Code Name:                          Haswell-EP
  CPU Technology:                         22 nm
  CPU S-Spec:                             SR1XK
  CPU Thermal Design Power (TDP):         145.0 W
  CPU Thermal Design Current (TDC):       176.0 A
  CPU Power Limits (Max):                 Power = 290.00 W, Time = 40.00 sec
  CPU Power Limit 1 (Long Duration)/Processor Base Power (PBP): Power = 145.00 W, Time = 1.00 sec [Unlocked]
  CPU Power Limit 2 (Short Duration)/Maximum Turbo Power (MTP): Power = 174.00 W, Time = 7.81 ms [Unlocked]
  Configurable TDP Level 1 (Down):        145.00 W (34.50 W - 290.00 W), 1900 MHz
  Current Configurable TDP Level:         Nominal (Legacy) [Unlocked]
  CPU Max. Junction Temperature (Tj,max): 78 °C
  CPU Type:                               Production Unit
  CPU Platform:                           Socket R3 (LGA2011-3)
  Microcode Update Revision:              44
  Number of CPU Cores:                    18
  Number of Logical CPUs:                 36
 [Operating Points]
  CPU MFM (Low Power):                    800.0 MHz = 8 x 100.0 MHz
  CPU LFM (Minimum):                      1200.0 MHz = 12 x 100.0 MHz
  CPU HFM (Base):                         2300.0 MHz = 23 x 100.0 MHz
  CPU Turbo Max:                          3800.0 MHz = 38 x 100.0 MHz [Unlocked]
  Turbo Ratio Limits:                     38x (1-24c)
  CPU Current:                            2273.2 MHz = 23 x 98.8 MHz @ 0.8203 V
  LLC/Ring Maximum:                       3000.0 MHz = 30.00 x 100.0 MHz
  LLC/Ring Current:                       2965.0 MHz = 30.00 x 98.8 MHz
  CPU Bus Type:                           Intel Direct Media Interface (DMI) v2.0
  Maximum DMI Link Speed:                 5.0 GT/s
  Current DMI Link Speed:                 5.0 GT/s
 [Cache and TLB]
  L1 Cache:                               Instruction: 18 x 32 KBytes, Data: 18 x 32 KBytes
  L2 Cache:                               Integrated: 18 x 256 KBytes
  L3 Cache:                               45 MBytes
  Instruction TLB:                        2MB/4MB Pages, Fully associative, 8 entries
  Data TLB:                               4 KB Pages, 4-way set associative, 64 entries
 [Standard Feature Flags]
  FPU on Chip                             Present
  Enhanced Virtual-86 Mode                Present
  I/O Breakpoints                         Present
  Page Size Extensions                    Present
  Time Stamp Counter                      Present
  Pentium-style Model Specific Registers  Present
  Physical Address Extension              Present
  Machine Check Exception                 Present
  CMPXCHG8B Instruction                   Present
  APIC On Chip / PGE (AMD)                Present
  Fast System Call                        Present
  Memory Type Range Registers             Present
  Page Global Feature                     Present
  Machine Check Architecture              Present
  CMOV Instruction                        Present
  Page Attribute Table                    Present
  36-bit Page Size Extensions             Present
  Processor Number                        Not Present
  CLFLUSH Instruction                     Present
  Debug Trace and EMON Store              Not Present
  Internal ACPI Support                   Present
  MMX Technology                          Present
  Fast FP Save/Restore (IA MMX-2)         Present
  Streaming SIMD Extensions               Present
  Streaming SIMD Extensions 2             Present
  Self-Snoop                              Present
  Multi-Threading Capable                 Present
  Automatic Clock Control                 Present
  IA-64 Processor                         Not Present
  Signal Break on FERR                    Present
  Virtual Machine Extensions (VMX)        Not Present
  Safer Mode Extensions (Intel TXT)       Not Present
  Streaming SIMD Extensions 3             Present
  Supplemental Streaming SIMD Extensions 3 Present
  Streaming SIMD Extensions 4.1           Present
  Streaming SIMD Extensions 4.2           Present
  AVX Support                             Present
  Fused Multiply Add (FMA)                Present
  Carryless Multiplication (PCLMULQDQ)/GFMUL Present
  CMPXCHG16B Support                      Present
  MOVBE Instruction                       Present
  POPCNT Instruction                      Present
  XSAVE/XRSTOR/XSETBV/XGETBV Instructions Present
  XGETBV/XSETBV OS Enabled                Present
  Float16 Instructions                    Present
  AES Cryptography Support                Present
  Random Number Read Instruction (RDRAND) Present
  Extended xAPIC                          Not Present
  MONITOR/MWAIT Support                   Present
  Thermal Monitor 2                       Present
  Enhanced SpeedStep Technology           Present
  L1 Context ID                           Not Present
  Send Task Priority Messages Disabling   Present
  Processor Context ID                    Present
  Direct Cache Access                     Not Present
  TSC-deadline Timer                      Present
  Performance/Debug Capability MSR        Present
  IA32 Debug Interface Support            Not Present
  64-Bit Debug Store                      Not Present
  CPL Qualified Debug Store               Not Present
 [Extended Feature Flags]
  64-bit Extensions                       Present
  RDTSCP and TSC_AUX Support              Present
  1 GB large page support                 Present
  No Execute                              Present
  SYSCALL/SYSRET Support                  Present
  Bit Manipulation Instructions Set 1     Present
  Bit Manipulation Instructions Set 2     Present
  Advanced Vector Extensions 2 (AVX2)     Present
  Advanced Vector Extensions 512 (AVX-512) Foundation Not Present
  AVX-512 Prefetch Instructions           Not Present
  AVX-512 Exponential and Reciprocal Instructions Not Present
  AVX-512 Conflict Detection Instructions Not Present
  AVX-512 Doubleword and Quadword Instructions Not Present
  AVX-512 Byte and Word Instructions      Not Present
  AVX-512 Vector Length Extensions        Not Present
  AVX-512 52-bit Integer FMA Instructions Not Present
  Secure Hash Algorithm (SHA) Extensions  Not Present
  Software Guard Extensions (SGX) Support Not Present
  Supervisor Mode Execution Protection (SMEP) Present
  Supervisor Mode Access Prevention (SMAP) Not Present
  Hardware Lock Elision (HLE)             Not Present
  Restricted Transactional Memory (RTM)   Not Present
  Memory Protection Extensions (MPX)      Not Present
  Read/Write FS/GS Base Instructions      Present
  Enhanced Performance String Instruction Present
  INVPCID Instruction                     Present
  RDSEED Instruction                      Not Present
  Multi-precision Add Carry Instructions (ADX) Not Present
  PCOMMIT Instructions                    Not Present
  CLFLUSHOPT Instructions                 Not Present
  CLWB Instructions                       Not Present
  TSC_THREAD_OFFSET                       Not Present
  Platform Quality of Service Monitoring (PQM) Present
  Platform Quality of Service Enforcement (PQE) Not Present
  FPU Data Pointer updated only on x87 Exceptions Not Present
  Deprecated FPU CS and FPU DS            Present
  Intel Processor Trace                   Not Present
  PREFETCHWT1 Instruction                 Not Present
  AVX-512 Vector Bit Manipulation Instructions Not Present
  AVX-512 Vector Bit Manipulation Instructions 2 Not Present
  AVX-512 Galois Fields New Instructions  Not Present
  AVX-512 Vector AES                      Not Present
  AVX-512 Vector Neural Network Instructions Not Present
  AVX-512 Bit Algorithms                  Not Present
  AVX-512 Carry-Less Multiplication Quadword (VPCLMULQDQ) Not Present
  AVX-512 Vector POPCNT (VPOPCNTD/VPOPCNTQ) Not Present
  User-Mode Instruction Prevention        Not Present
  Protection Keys for User-mode Pages     Not Present
  OS Enabled Protection Keys              Not Present
  Wait and Pause Enhancements (WAITPKG)   Not Present
  Total Memory Encryption                 Not Present
  Key Locker                              Not Present
  57-bit Linear Addresses, 5-level Paging Not Present
  Read Processor ID                       Not Present
  Cache Line Demote                       Not Present
  MOVDIRI: Direct Stores                  Not Present
  MOVDIR64B: Direct Stores                Not Present
  ENQCMD: Enqueue Stores                  Not Present
  SGX Launch Configuration                Not Present
  Protection Keys for Supervisor-Mode Pages Not Present
  Control-Flow Enforcement Technology (CET) Shadow Stack Not Present
  AVX-512 4 x Vector Neural Network Instructions Word Variable Precision Not Present
  AVX-512 4 x Fused Multiply Accumulation Packed Single Precision Not Present
  Fast Short REP MOV                      Not Present
  User Interrupts                         Not Present
  AVX-512 VP2INTERSECT Support            Not Present
  AVX-512 FP16                            Not Present
  MD_CLEAR Support                        Present
  Restricted Transactional Memory (RTM) Always Abort Not Present
  SERIALIZE                               Not Present
  Hybrid Processor                        Not Present
  TSX Suspend Load Address Tracking       Not Present
  Platform Configuration (PCONFIG)        Not Present
  Indirect Branch Restricted Speculation (IBRS), Indirect Branch Predictor Barrier (IBPB) Present
  Single Thread Indirect Branch Predictors (STIBP) Present
  L1D_FLUSH Support                       Present
  IA32_ARCH_CAPABILITIES MSR              Present
  IA32_CORE_CAPABILITIES MSR              Not Present
  Speculative Store Bypass Disable (SSBD) Present
  Control-Flow Enforcement Technology (CET) Indirect Branch Tracking Not Present
  Advanced Matrix Extensions (AMX) Tile Architecture Not Present
  Advanced Matrix Extensions (AMX) bfloat16 Support Not Present
  Advanced Matrix Extensions (AMX) 8-bit Integer Operations Not Present
  AVX (VEX-encoded) Vector Neural Network Instructions Not Present
  AVX-512 BFLOAT16 Instructions           Not Present
  Fast Zero-Length MOVSB                  Not Present
  Fast Short STOSB                        Not Present
  Fast Short CMPSB, SCASB                 Not Present
  History Reset                           Not Present
  Linear Address Masking                  Not Present
  Protected Processor Inventory Number (IA32_PPIN) Support Not Present
 [Vulnerability Mitigation Mechanisms]
  Rogue Data Cache Load (RDCL)            Susceptible
  Speculative Store Bypass (SSB)          Susceptible
  Microarchitectural Data Sampling (MDS)  Susceptible
  MCE on modifying code page size without TLB invalidation Susceptible
  Transactional Asynchronous Abort (TAA)  Affected
  Indirect Branch Restriction Speculation (IBRS) Not Supported
  RSB Alternate                           Not Supported
  L1D Flush on VM Entry Not Needed        Not Supported
  Energy Filtering Control                Not Supported
 [Enhanced Features]
  Thermal Monitor 1:                      Supported, Enabled
  Thermal Monitor 2:                      Supported, Enabled
  Enhanced Intel SpeedStep (GV3):         Supported, Enabled
  Bi-directional PROCHOT#:                Enabled
  Extended Auto-HALT State C1E:           Enabled
  MLC Streamer Prefetcher                 Supported, Enabled
  MLC Spatial Prefetcher                  Supported, Enabled
  DCU Streamer Prefetcher                 Supported, Enabled
  DCU IP Prefetcher                       Supported, Enabled
  Intel Dynamic Acceleration (IDA) Technology: Not Supported
  Intel Dynamic FSB Switching:            Not Supported
  Intel Turbo Boost Technology:           Supported, Enabled
  Programmable Ratio Limits:              Supported, Disabled
  Programmable TDC/TDP Limits:            Supported, Disabled
  Hardware Duty Cycling:                  Not Supported
  Intel Speed Select:                     Not Supported
 [CPU Scalable Features]
  GSSE256 Instructions:                   Enabled
  AES:                                    Enabled
  LT SX (TXT for Servers):                Enabled
  LT Production:                          Enabled
  SMX:                                    Enabled
  VMX:                                    Enabled
  VT-x3:                                  Enabled
  VT Real Mode:                           Disabled
  VT CPAUSE:                              Disabled
  Multi-Threading (HT):                   Enabled
  Programmable TDP Limits:                Enabled
  EX Config:                              Disabled
  EP 4S Config:                           Disabled
  EP (1S/2S) Config:                      Enabled
  EN (1S/2S) Config:                      Disabled
  UP (1S/WS) Config:                      Disabled
  Memory Channel Mirroring Mode:          Enabled
  Memory LT Support:                      Enabled
  Memory Frequency Support:               DDR-1867
  Physical Address Size Supported (Core): 46-bit
  Extended APIC (x2APIC):                 Enabled
  CPU HOT ADD:                            Disabled
  GV3:                                    Enabled
  Core RAS (Data Poisoning, MCA Recovery): Enabled
  DCA:                                    Enabled
  QPI Link 2:                             Disabled
  QPI Link 1:                             Enabled
  QPI Link 0:                             Enabled
  Maximum Supported QPI Ratio:            9.6 GT/s
  NTB:                                    Enabled
  RAID-on-load:                           Enabled
  PCIe LT SX:                             Enabled
  PCIe LT:                                Enabled
  PCIe Gen 3:                             Enabled
  PCIe DMA:                               Enabled
  DMI:                                    Enabled
  DDR4:                                   Disabled
  Monroe Technology:                      Enabled
  SMBus Write Capability:                 Enabled
  Extended Addressing DIMM:               Enabled
  Extended Latency DIMM:                  Enabled
  Patrol Scrub:                           Enabled
  Rank Sparing:                           Enabled
  UDIMM Support:                          Enabled
  RDIMM Support:                          Enabled
  DIR:                                    Enabled
  ECC:                                    Enabled
  QR DIMM:                                Enabled
  LOCKSTEP:                               Enabled
  CLTT:                                   Enabled
  3N Mode:                                Enabled
  4Gb DDR3:                               Enabled
  8Gb DDR3:                               Enabled
  Memory Channel 0:                       Enabled
  Memory Channel 1:                       Enabled
  Memory Channel 2:                       Enabled
  Memory Channel 3:                       Enabled
  Intel SMI 2:                            Disabled
  CPU Stepping:                           C1
  DRAM Power Meter:                       Enabled
  DRAM RAPL:                              Enabled
  Overclocking:                           Disabled
  Energy Efficient Turbo:                 Enabled
  Per-core P-states:                      Enabled
  Uncore Frequency Scaling (UFS):         Enabled
  System Agent Power Management (SAPM) Dynamic Load Line (DLL): Enabled
  Targeted SMI:                           Enabled
  SMM CPU Save/Restore:                   Enabled
  SMM Code Access Check:                  Enabled
  Enhanced MCA:                           Enabled
  FMA Instructions:                       Enabled
  Hardware Lock Elison (HLE):             Enabled
  Hardware Lock Elison+ (HLE+)/RTM:       Enabled
  Cache Allocation Technology (CAT):      Disabled
  Cache Monitoring Technology (CMT):      Enabled
  Voltage Override Overclocking:          Enabled
  BCLK Coarse Ratio Support (PCIe Ratio Changing): Disabled
  Physical Chop:                          High-Core Count (HCC)
  Product Type:                           Haswell
  PCIE Ratio Change:                      Disabled
  VMCS Shadowing:                         Enabled
  FIT Boot:                               Enabled
  PFAT:                                   Disabled
  Error Spoofing:                         Disabled
  COD:                                    Enabled
  Haswell New Instructions:               Enabled
  Second Home Agent:                      Enabled
 [Memory Ranges]
  Maximum Physical Address Size:          46-bit (64 TBytes)
  Maximum Virtual Address Size:           48-bit (256 TBytes)
 [MTRRs]
  Range 80000000-100000000 (2048MB-4096MB) Type: Uncacheable (UC)
  Range 380000000000-384000000000 (58720256MB-58982400MB) Type: Uncacheable (UC)

Motherboard ---------------------------------------------------------------

 [Computer]
  Computer Brand Name:                    Acidanthera iMacPro1,1
 [Motherboard]
  Motherboard Model:                      Acidanthera Mac-7BA5B2D9E42DDD94
  Motherboard Chipset:                    Intel C612 (Wellsburg-G)
  Motherboard Slots:                      3xPCI Express x1, 1xPCI Express x4, 1xPCI Express x8, 2xPCI Express x16
  PCI Express Version Supported:          v3.0
  USB Version Supported:                  v3.0
 [BIOS]
  BIOS Manufacturer:                      Acidanthera
  BIOS Date:                              05/21/2022
  BIOS Version:                           1916.0.3.0.0
  UEFI BIOS:                              Capable
  Super-IO/LPC Chip:                      Nuvoton NCT6779D
  Trusted Platform Module (TPM) Chip:     Not Found

ACPI Devices --------------------------------------------------------------


Programmable interrupt controller -----------------------------------------

  Device Name:                            Programmable interrupt controller
 [Assigned Resources]
  I/O Port:                               0020 - 003D
 [Alternative 1]
  I/O Port:                               0020 - 003D
  I/O Port:                               00A0 - 00BD
  I/O Port:                               04D0 - 04D1

Advanced programmable interrupt controller --------------------------------

  Device Name:                            Advanced programmable interrupt controller
 [Assigned Resources]
  Memory Location:                        FEC00000 - FECFFFFF
 [Alternative 1]
  Memory Location:                        FEC00000 - FECFFFFF

System timer --------------------------------------------------------------

  Device Name:                            System timer
 [Assigned Resources]
  I/O Port:                               0040 - 0043
 [Alternative 1]
  I/O Port:                               0040 - 0043
  I/O Port:                               0050 - 0053

High precision event timer ------------------------------------------------

  Device Name:                            High precision event timer
 [Assigned Resources]
  IRQ:                                    0
 [Alternative 1]
  Memory Location:                        FED00000
  IRQ:                                    0
  IRQ:                                    8
  IRQ:                                    11

Direct memory access controller -------------------------------------------

  Device Name:                            Direct memory access controller
 [Assigned Resources]
  I/O Port:                               0000 - 000F
  I/O Port:                               008F
  Memory Location:                        00000000 - 00000086
 [Alternative 1]
  I/O Port:                               0000 - 000F
  I/O Port:                               0081 - 0083
  I/O Port:                               0087
  I/O Port:                               0089 - 008B
  I/O Port:                               008F
  I/O Port:                               00C0 - 00DF
  DMA:                                    4

Standard PS/2 Keyboard ----------------------------------------------------

  Device Name:                            Standard PS/2 Keyboard
 [Assigned Resources]
  I/O Port:                               0060
  I/O Port:                               0000
 [Alternative 1]
  I/O Port:                               0060
  I/O Port:                               0064
  IRQ:                                    1

Communications Port -------------------------------------------------------

  Device Name:                            Communications Port
 [Assigned Resources]
  I/O Port:                               03F8 - 03FF
 [Alternative 1]
  I/O Port:                               03F8 - 03FF
  IRQ:                                    4
 [Alternative 2]
  I/O Port:                               03F8 - 03FF
  IRQ:                                    3
  IRQ:                                    4
  IRQ:                                    5
  IRQ:                                    7
  IRQ:                                    9
  IRQ:                                    10
  IRQ:                                    11
  IRQ:                                    12
 [Alternative 3]
  I/O Port:                               02F8 - 02FF
  IRQ:                                    3
  IRQ:                                    4
  IRQ:                                    5
  IRQ:                                    7
  IRQ:                                    9
  IRQ:                                    10
  IRQ:                                    11
  IRQ:                                    12
 [Alternative 4]
  I/O Port:                               03E8 - 03EF
  IRQ:                                    3
  IRQ:                                    4
  IRQ:                                    5
  IRQ:                                    7
  IRQ:                                    9
  IRQ:                                    10
  IRQ:                                    11
  IRQ:                                    12
 [Alternative 5]
  I/O Port:                               02E8 - 02EF
  IRQ:                                    3
  IRQ:                                    4
  IRQ:                                    5
  IRQ:                                    7
  IRQ:                                    9
  IRQ:                                    10
  IRQ:                                    11
  IRQ:                                    12

System speaker ------------------------------------------------------------

  Device Name:                            System speaker
 [Assigned Resources]
  I/O Port:                               0061
 [Alternative 1]
  I/O Port:                               0061

PCI Bus -------------------------------------------------------------------

  Device Name:                            PCI Bus
 [Assigned Resources]
 [Alternative 1]

PCI Express Root Complex --------------------------------------------------

  Device Name:                            PCI Express Root Complex
 [Assigned Resources]
  I/O Port:                               0000 - FFFFFFFF
  Memory Location:                        000A0000 - 000BFFFF
 [Alternative 1]
  I/O Port:                               0000 - 0CF7
  I/O Port:                               1000 - FFFF
  Memory Location:                        000A0000 - 000BFFFF
  Memory Location:                        90000000 - FBFFBFFF

System CMOS/real time clock -----------------------------------------------

  Device Name:                            System CMOS/real time clock
 [Assigned Resources]
  I/O Port:                               0070 - 0071
 [Alternative 1]
  I/O Port:                               0070 - 0071
  I/O Port:                               0074 - 0077

Motherboard resources -----------------------------------------------------

  Device Name:                            Motherboard resources
 [Assigned Resources]
  I/O Port:                               0A00 - 0A0F
 [Alternative 1]
  I/O Port:                               0A00 - 0A0F
  I/O Port:                               0A10 - 0A1F
  I/O Port:                               0A20 - 0A2F
  I/O Port:                               0A30 - 0A3F

Motherboard resources -----------------------------------------------------

  Device Name:                            Motherboard resources
 [Assigned Resources]
  I/O Port:                               0500 - 057F
  I/O Port:                               0072 - 0073
  I/O Port:                               0000 - 0083
  I/O Port:                               008C - 008E
  I/O Port:                               0880 - 0883
  Memory Location:                        FF000000 - FFFFFFFF
 [Alternative 1]
  I/O Port:                               0500 - 057F
  I/O Port:                               0400 - 047F
  I/O Port:                               0092
  I/O Port:                               0010 - 001F
  I/O Port:                               0072 - 0073
  I/O Port:                               0080
  I/O Port:                               0084 - 0086
  I/O Port:                               0088
  I/O Port:                               008C - 008E
  I/O Port:                               0090 - 009F
  I/O Port:                               0580 - 059F
  I/O Port:                               0600 - 061F
  I/O Port:                               0880 - 0883
  I/O Port:                               0800 - 081F
  Memory Location:                        FED1C000 - FED3FFFF
  Memory Location:                        FED45000 - FED8BFFF
  Memory Location:                        FF000000
  Memory Location:                        FEE00000 - FEEFFFFF
  Memory Location:                        FED12000 - FED1200F
  Memory Location:                        FED12010
  Memory Location:                        FED1B000 - FED1BFFF

Numeric data processor ----------------------------------------------------

  Device Name:                            Numeric data processor
 [Assigned Resources]
  I/O Port:                               00F0
 [Alternative 1]
  I/O Port:                               00F0
  IRQ:                                    13

Microsoft PS/2 Mouse ------------------------------------------------------

  Device Name:                            Microsoft PS/2 Mouse
 [Assigned Resources]
  IRQ:                                    12
 [Alternative 1]
  IRQ:                                    12

SMBIOS DMI ----------------------------------------------------------------


BIOS ----------------------------------------------------------------------

  BIOS Vendor:                            Acidanthera
  BIOS Version:                           1916.0.3.0.0
  BIOS Release Date:                      05/21/2022
  BIOS Start Segment:                     0
  BIOS Size:                              0 MBytes
  System BIOS Version:                    5.11
  ISA Support:                            Not Present
  MCA Support:                            Not Present
  EISA Support:                           Not Present
  PCI Support:                            Present
  PC Card (PCMCIA) Support:               Not Present
  Plug-and-Play Support:                  Not Present
  APM Support:                            Not Present
  Flash BIOS:                             Present
  BIOS Shadow:                            Present
  VL-VESA Support:                        Not Present
  ESCD Support:                           Not Present
  Boot from CD:                           Present
  Selectable Boot:                        Present
  BIOS ROM Socketed:                      Present
  Boot from PC Card:                      Not Present
  EDD Support:                            Present
  NEC PC-98 Support:                      Not Present
  ACPI Support:                           Present
  USB Legacy Support:                     Present
  AGP Support:                            Not Present
  I2O Boot Support:                       Not Present
  LS-120 Boot Support:                    Not Present
  ATAPI ZIP Drive Boot Support:           Not Present
  IEE1394 Boot Support:                   Not Present
  Smart Battery Support:                  Not Present
  BIOS Boot Specification Support:        Present
  Function key-initiated Network Service Boot Support: Not Present
  Targeted Content Distribution Support:  Present
  UEFI Specification Support:             Present
  Virtual Machine:                        Not Present

System --------------------------------------------------------------------

  System Manufacturer:                    Acidanthera
  Product Name:                           iMacPro1,1
  Product Version:                        1.0
  Product Serial Number:                  C02YM0CLHX87
  UUID:                                   {6485EA46-23C8-4B57-AFF0-3E395B2B9F5B}
  SKU Number:                             
  Family:                                 iMac Pro

Mainboard -----------------------------------------------------------------

  Mainboard Manufacturer:                 Acidanthera
  Mainboard Name:                         Mac-7BA5B2D9E42DDD94
  Mainboard Version:                      iMacPro1,1
  Mainboard Serial Number:                C02917401GUJG36AD
  Asset Tag:                              
  Location in chassis:                    

System Enclosure ----------------------------------------------------------

  Manufacturer:                           Acidanthera
  Case Type:                              All in One
  Version:                                Mac-7BA5B2D9E42DDD94
  Serial Number:                          C02YM0CLHX87
  Asset Tag Number:                       

CPU Internal L1 -----------------------------------------------------------

  Socket Designation:                     CPU Internal L1
  Cache State:                            Enabled
  Cache Location:                         Internal
  Cache Type:                             L1
  Cache Scheme:                           Write-Back
  Supported SRAM Type:                    
  Current SRAM Type:                      
  Cache Speed:                            Unknown
  Error Correction Type:                  Parity
  Maximum Cache Size:                     1152 KBytes
  Installed Cache Size:                   Parity
  Cache Associativity:                    8-way Set-Associative

CPU Internal L2 -----------------------------------------------------------

  Socket Designation:                     CPU Internal L2
  Cache State:                            Enabled
  Cache Location:                         Internal
  Cache Type:                             L2 Unified
  Cache Scheme:                           Write-Back
  Supported SRAM Type:                    
  Current SRAM Type:                      
  Cache Speed:                            Unknown
  Error Correction Type:                  Single-bit ECC
  Maximum Cache Size:                     4608 KBytes
  Installed Cache Size:                   Single-bit ECC
  Cache Associativity:                    8-way Set-Associative

CPU Internal L3 -----------------------------------------------------------

  Socket Designation:                     CPU Internal L3
  Cache State:                            Enabled
  Cache Location:                         Internal
  Cache Type:                             L3 Unified
  Cache Scheme:                           Write-Back
  Supported SRAM Type:                    
  Current SRAM Type:                      
  Cache Speed:                            Unknown
  Error Correction Type:                  Single-bit ECC
  Maximum Cache Size:                     46080 KBytes
  Installed Cache Size:                   Single-bit ECC
  Cache Associativity:                    20-way Set-Associative

Processor -----------------------------------------------------------------

  Processor Manufacturer:                 Intel
  Processor Version:                      Intel(R) Xeon(R) CPU E5-2696 v3 @ 2.30GHz
  External Clock:                         100 MHz
  Maximum Clock Supported:                2300 MHz
  Current Clock:                          2300 MHz
  CPU Socket:                             Populated
  CPU Status:                             Enabled
  Processor Type:                         Central Processor
  Processor Voltage:                      0.2 V
  Processor Upgrade:                      Socket LGA2011-3
  Socket Designation:                     SOCKET 0

System Boot Information ---------------------------------------------------

  Boot Status:                            No error occurred

NIC -----------------------------------------------------------------------


Memory Devices ------------------------------------------------------------


Physical Memory Array -----------------------------------------------------

  Array Location:                         System board
  Array Use:                              System memory
  Error Detecting Method:                 Multi-bit ECC
  Memory Capacity:                        256 GBytes
  Memory Devices:                         4

Memory Array Mapped Address -----------------------------------------------

  Starting Address:                       00000000
  Ending Address:                         01FFFFFF
  Partition Width:                        1

Memory Device -------------------------------------------------------------

  Total Width:                            72 bits
  Data Width:                             72 bits
  Device Size:                            32768 MBytes
  Device Form Factor:                     DIMM
  Device Locator:                         DIMM_A1
  Bank Locator:                           NODE 1
  Device Type:                            DDR3 SDRAM
  Device Type Detail:                     Synchronous
  Memory Speed:                           1867 MHz
  Manufacturer:                           Hynix Semiconductor
  Serial Number:                          4024E093
  Part Number:                            HMT84GL7AMR4C-RD
  Asset Tag:                              DIMM_A1_AssetTag

Memory Device Mapped Address ----------------------------------------------

  Starting Address:                       00000000
  Ending Address:                         01FFFFFF
  Partition Row Position:                 1
  Interleave Position:                    Non-interleaved
  Interleave Data Depth:                  0

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Physical Memory Array -----------------------------------------------------

  Array Location:                         System board
  Array Use:                              System memory
  Error Detecting Method:                 Multi-bit ECC
  Memory Capacity:                        256 GBytes
  Memory Devices:                         4

Memory Array Mapped Address -----------------------------------------------

  Starting Address:                       02000000
  Ending Address:                         03FFFFFF
  Partition Width:                        1

Memory Device -------------------------------------------------------------

  Total Width:                            72 bits
  Data Width:                             72 bits
  Device Size:                            32768 MBytes
  Device Form Factor:                     DIMM
  Device Locator:                         DIMM_C1
  Bank Locator:                           NODE 2
  Device Type:                            DDR3 SDRAM
  Device Type Detail:                     Synchronous
  Memory Speed:                           1867 MHz
  Manufacturer:                           Hynix Semiconductor
  Serial Number:                          4051B36C
  Part Number:                            HMT84GL7AMR4C-RD
  Asset Tag:                              DIMM_C1_AssetTag

Memory Device Mapped Address ----------------------------------------------

  Starting Address:                       02000000
  Ending Address:                         03FFFFFF
  Partition Row Position:                 1
  Interleave Position:                    Non-interleaved
  Interleave Data Depth:                  0

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Physical Memory Array -----------------------------------------------------

  Array Location:                         System board
  Array Use:                              System memory
  Error Detecting Method:                 Multi-bit ECC
  Memory Capacity:                        256 GBytes
  Memory Devices:                         4

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Physical Memory Array -----------------------------------------------------

  Array Location:                         System board
  Array Use:                              System memory
  Error Detecting Method:                 Multi-bit ECC
  Memory Capacity:                        256 GBytes
  Memory Devices:                         4

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Memory Device -------------------------------------------------------------

  Total Width:                            0 bits
  Data Width:                             0 bits
  Device Size:                            0 MBytes
  Device Form Factor:                     Unknown
  Device Locator:                         NO DIMM
  Bank Locator:                           NO DIMM
  Device Type:                            Unknown
  Device Type Detail:                     
  Manufacturer:                           NO DIMM
  Serial Number:                          NO DIMM
  Part Number:                            NO DIMM
  Asset Tag:                              NO DIMM

Port Connectors -----------------------------------------------------------


Mouse Port ----------------------------------------------------------------

  Port Type:                              Mouse Port
  Internal Reference:                     J1A1
  Internal Connector Type:                None
  External Reference:                     PS2Mouse
  External Connector Type:                PS/2

Keyboard Port -------------------------------------------------------------

  Port Type:                              Keyboard Port
  Internal Reference:                     J1A1
  Internal Connector Type:                None
  External Reference:                     Keyboard
  External Connector Type:                PS/2

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J2A1
  Internal Connector Type:                None
  External Reference:                     TV Out
  External Connector Type:                Mini-Centronics Type-14

Serial Port 16550A Compatible ---------------------------------------------

  Port Type:                              Serial Port 16550A Compatible
  Internal Reference:                     J2A2A
  Internal Connector Type:                None
  External Reference:                     COM A
  External Connector Type:                DB-9 pin male

Video Port ----------------------------------------------------------------

  Port Type:                              Video Port
  Internal Reference:                     J2A2B
  Internal Connector Type:                None
  External Reference:                     Video
  External Connector Type:                DB-15 pin female

USB -----------------------------------------------------------------------

  Port Type:                              USB
  Internal Reference:                     J3A1
  Internal Connector Type:                None
  External Reference:                     USB1
  External Connector Type:                Access Bus (USB)

USB -----------------------------------------------------------------------

  Port Type:                              USB
  Internal Reference:                     J3A1
  Internal Connector Type:                None
  External Reference:                     USB2
  External Connector Type:                Access Bus (USB)

USB -----------------------------------------------------------------------

  Port Type:                              USB
  Internal Reference:                     J3A1
  Internal Connector Type:                None
  External Reference:                     USB3
  External Connector Type:                Access Bus (USB)

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9A1 - TPM HDR
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9C1 - PCIE DOCKING CONN
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J2B3 - CPU FAN
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J6C2 - EXT HDMI
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J3C1 - GMCH FAN
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J1D1 - ITP
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9E2 - MDC INTPSR
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9E4 - MDC INTPSR
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9E3 - LPC HOT DOCKING
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9E1 - SCAN MATRIX
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J9G1 - LPC SIDE BAND
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J8F1 - UNIFIED
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J6F1 - LVDS
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J2F1 - LAI FAN
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J2G1 - GFX VID
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

Port Connector ------------------------------------------------------------

  Port Type:                              Unknown
  Internal Reference:                     J1G6 - AC JACK
  Internal Connector Type:                Unknown
  External Reference:                     
  External Connector Type:                None

System Slots --------------------------------------------------------------


Slot1 ---------------------------------------------------------------------

  Slot Designation:                       Slot1
  Slot Type:                              PCI Express Gen3 x1
  Slot Usage:                             Empty
  Slot Data Bus Width:                    1x / x1
  Slot Length:                            Short
  Base Bus:Device:Function Number:        3:0:3

Slot2 ---------------------------------------------------------------------

  Slot Designation:                       Slot2
  Slot Type:                              PCI Express Gen3 x8
  Slot Usage:                             Empty
  Slot Data Bus Width:                    8x / x8
  Slot Length:                            Short
  Base Bus:Device:Function Number:        1:0:0

Slot3 ---------------------------------------------------------------------

  Slot Designation:                       Slot3
  Slot Type:                              PCI Express Gen3 x1
  Slot Usage:                             Empty
  Slot Data Bus Width:                    1x / x1
  Slot Length:                            Short
  Base Bus:Device:Function Number:        -:0:0

Slot4 ---------------------------------------------------------------------

  Slot Designation:                       Slot4
  Slot Type:                              PCI Express Gen3 x16
  Slot Usage:                             Empty
  Slot Data Bus Width:                    16x / x16
  Slot Length:                            Long
  Base Bus:Device:Function Number:        -:0:0

Slot5 ---------------------------------------------------------------------

  Slot Designation:                       Slot5
  Slot Type:                              PCI Express Gen3 x4
  Slot Usage:                             Empty
  Slot Data Bus Width:                    4x / x4
  Slot Length:                            Short
  Base Bus:Device:Function Number:        -:0:4

Slot6 ---------------------------------------------------------------------

  Slot Designation:                       Slot6
  Slot Type:                              PCI Express Gen3 x16
  Slot Usage:                             Empty
  Slot Data Bus Width:                    16x / x16
  Slot Length:                            Long
  Base Bus:Device:Function Number:        1:0:0

Slot7 ---------------------------------------------------------------------

  Slot Designation:                       Slot7
  Slot Type:                              PCI Express Gen3 x1
  Slot Usage:                             Empty
  Slot Data Bus Width:                    1x / x1
  Slot Length:                            Short
  Base Bus:Device:Function Number:        -:0:1

Memory --------------------------------------------------------------------

 [General Information]
  Total Memory Size:                      64 GBytes
  Total Memory Size [MB]:                 65536
 [Current Performance Settings]
  Maximum Supported Memory Clock:         933.3 MHz
  Current Memory Clock:                   922.5 MHz
  Current Timing (tCAS-tRCD-tRP-tRAS):    13-13-13-32
  Memory Channels Supported:              4
  Memory Channels Active:                 2
  Command Rate (CR):                      1T
  Read to Read Delay (tRDRD_DG/TrdrdScDlr) Different Bank Group: 1T
  Read to Read Delay (tRDRD_DD) Different DIMM: 4T
  Write to Write Delay (tWRWR_DG/TwrwrScDlr) Different Bank Group: 3T
  Write to Write Delay (tWRWR_DD) Different DIMM: 3T
  Read to Write Delay (tRDWR_SG/TrdwrScL) Same Bank Group: 7T
  Read to Write Delay (tRDWR_DD) Different DIMM: 2T
  Write to Read Delay (tWRRD_DD) Different DIMM: 2T
  Read to Precharge Delay (tRTP):         7T
  Write to Precharge Delay (tWTP):        25T
  Write Recovery Time (tWR):              14T
  RAS# to RAS# Delay (tRRD):              5T
  Refresh Cycle Time (tRFC):              243T
  Four Activate Window (tFAW):            26T

Row: 0 [NODE 1/DIMM_A1] - 32 GB PC3-14900 DDR3 SDRAM SK Hynix HMT84GL7AMR4C-RD

 [General Module Information]
  Module Number:                          0
  Module Size:                            32 GBytes
  Memory Type:                            DDR3 SDRAM
  Module Type:                            LRDIMM
  Memory Speed:                           933.7 MHz (DDR3-1867 / PC3-14900)
  Module Manufacturer:                    SK Hynix
  Module Part Number:                     HMT84GL7AMR4C-RD
  Module Revision:                        17229
  Module Serial Number:                   2480940096 (4024E093)
  Module Manufacturing Date:              Year: 2014, Week: 14
  Module Manufacturing Location:          1
  SDRAM Manufacturer:                     SK Hynix
  Error Check/Correction:                 ECC
 [Module characteristics]
  Row Address Bits:                       16
  Column Address Bits:                    11
  Number Of Banks:                        8
  Module Density:                         4096 Mb
  Number Of Ranks:                        4
  Device Width:                           4 bits
  Bus Width:                              64 bits
  Module Nominal Voltage (VDD):           1.5 V
 [Module timing]
  Minimum SDRAM Cycle Time (tCKmin):      1.071 ns
  CAS# Latencies Supported:               6, 7, 8, 9, 10, 11, 13
  Minimum CAS# Latency Time (tAAmin):     13.125 ns
  Minimum RAS# to CAS# Delay (tRCDmin):   13.125 ns
  Minimum Row Precharge Time (tRPmin):    13.125 ns
  Minimum Active to Precharge Time (tRASmin): 34.000 ns
  Supported Module Timing at 933.3 MHz:   13-13-13-32
  Supported Module Timing at 800.0 MHz:   11-11-11-28
  Supported Module Timing at 666.7 MHz:   9-9-9-23
  Supported Module Timing at 533.3 MHz:   7-7-7-19
  Supported Module Timing at 400.0 MHz:   6-6-6-14
  Minimum Write Recovery Time (tWRmin):   15.000 ns
  Minimum Row Active to Row Active Delay (tRRDmin): 5.000 ns
  Minimum Active to Active/Refresh Time (tRCmin): 47.125 ns
  Minimum Refresh Recovery Time Delay (tRFCmin): 260.000 ns
  Minimum Internal Write to Read Command Delay (tWTRmin): 7.500 ns
  Minimum Internal Read to Precharge Command Delay (tRTPmin): 7.500 ns
  Minimum Four Activate Window Delay Time (tFAWmin): 27.000 ns
 [Features]
  Partial Array Self Refresh (PASR):      Not Supported
  On-die Thermal Sensor (ODTS) Readout:   Not Supported
  Auto Self Refresh (ASR):                Not Supported
  Extended Temperature 1X Refresh Rate:   Not Supported
  Extended Temperature Range:             Supported
  Module Temperature Sensor:              Supported
  Pseudo Target Row Refresh (pTRR):       Supported
  Maximum Active Window (MAW):            64 mS
  Unlimited MAC:                          Not Supported
  Maximum Active Window (MAW):            400K
  Module Nominal Height:                  30 - 31 mm
  Module Maximum Thickness (Front):       3 - 4 mm
  Module Maximum Thickness (Back):        3 - 4 mm

Row: 16 [NODE 2/DIMM_C1] - 32 GB PC3-14900 DDR3 SDRAM SK Hynix HMT84GL7AMR4C-RD

 [General Module Information]
  Module Number:                          16
  Module Size:                            32 GBytes
  Memory Type:                            DDR3 SDRAM
  Module Type:                            LRDIMM
  Memory Speed:                           933.7 MHz (DDR3-1867 / PC3-14900)
  Module Manufacturer:                    SK Hynix
  Module Part Number:                     HMT84GL7AMR4C-RD
  Module Revision:                        17229
  Module Serial Number:                   1823691072 (4051B36C)
  Module Manufacturing Date:              Year: 2014, Week: 32
  Module Manufacturing Location:          1
  SDRAM Manufacturer:                     SK Hynix
  Error Check/Correction:                 ECC
 [Module characteristics]
  Row Address Bits:                       16
  Column Address Bits:                    11
  Number Of Banks:                        8
  Module Density:                         4096 Mb
  Number Of Ranks:                        4
  Device Width:                           4 bits
  Bus Width:                              64 bits
  Module Nominal Voltage (VDD):           1.5 V
 [Module timing]
  Minimum SDRAM Cycle Time (tCKmin):      1.071 ns
  CAS# Latencies Supported:               6, 7, 8, 9, 10, 11, 13
  Minimum CAS# Latency Time (tAAmin):     13.125 ns
  Minimum RAS# to CAS# Delay (tRCDmin):   13.125 ns
  Minimum Row Precharge Time (tRPmin):    13.125 ns
  Minimum Active to Precharge Time (tRASmin): 34.000 ns
  Supported Module Timing at 933.3 MHz:   13-13-13-32
  Supported Module Timing at 800.0 MHz:   11-11-11-28
  Supported Module Timing at 666.7 MHz:   9-9-9-23
  Supported Module Timing at 533.3 MHz:   7-7-7-19
  Supported Module Timing at 400.0 MHz:   6-6-6-14
  Minimum Write Recovery Time (tWRmin):   15.000 ns
  Minimum Row Active to Row Active Delay (tRRDmin): 5.000 ns
  Minimum Active to Active/Refresh Time (tRCmin): 47.125 ns
  Minimum Refresh Recovery Time Delay (tRFCmin): 260.000 ns
  Minimum Internal Write to Read Command Delay (tWTRmin): 7.500 ns
  Minimum Internal Read to Precharge Command Delay (tRTPmin): 7.500 ns
  Minimum Four Activate Window Delay Time (tFAWmin): 27.000 ns
 [Features]
  Partial Array Self Refresh (PASR):      Not Supported
  On-die Thermal Sensor (ODTS) Readout:   Not Supported
  Auto Self Refresh (ASR):                Not Supported
  Extended Temperature 1X Refresh Rate:   Not Supported
  Extended Temperature Range:             Supported
  Module Temperature Sensor:              Supported
  Pseudo Target Row Refresh (pTRR):       Supported
  Maximum Active Window (MAW):            64 mS
  Unlimited MAC:                          Not Supported
  Maximum Active Window (MAW):            400K
  Module Nominal Height:                  30 - 31 mm
  Module Maximum Thickness (Front):       3 - 4 mm
  Module Maximum Thickness (Back):        3 - 4 mm

Bus -----------------------------------------------------------------------


PCI Bus #0 ----------------------------------------------------------------


Intel Haswell-EN/EP/EP 4S/EX IIO - DMI2 Port (x4) -------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - DMI2 Port (x4)
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - DMI2 Port (x4)
  Device Class:                           Host-to-PCI Bridge
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F00&SUBSYS_00008086&REV_02
 [PCI Express]
  Version:                                2.0
  Maximum Link Width:                     4x
  Current Link Width:                     Not negotiated
  Maximum Link Speed:                     5.0 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        8 - 16 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI standard host CPU bridge
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F00&SUBSYS_00008086&REV_02\3&11583659&0&00
  Location Paths                          PCIROOT(0)#PCI(0000)

Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4) --------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4)
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4)
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:1:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F02&SUBSYS_00000000&REV_02
 [PCI Express]
  Version:                                3.0
  Maximum Link Width:                     4x
  Current Link Width:                     Not negotiated
  Maximum Link Speed:                     8.0 GT/s
  Current Link Speed:                     2.5 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       Yes
  Hot-Plug:                               Not Capable
  Hot-Plug Surprise:                      Not Capable
  Slot Power Limit:                       26.000 W
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        8 - 16 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Root Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F02&SUBSYS_00008086&REV_02\3&11583659&0&08
  Location Paths                          PCIROOT(0)#PCI(0100)

PCI Express x4 Bus #1 -----------------------------------------------------


Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4) --------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4)
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 1 (x8/x4)
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:1:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F03&SUBSYS_00000000&REV_02
 [PCI Express]
  Version:                                3.0
  Maximum Link Width:                     4x
  Current Link Width:                     4x
  Maximum Link Speed:                     8.0 GT/s
  Current Link Speed:                     8.0 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        8 - 16 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Root Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F03&SUBSYS_00008086&REV_02\3&11583659&0&09
  Location Paths                          PCIROOT(0)#PCI(0101)

PCI Express x4 Bus #2 -----------------------------------------------------


Samsung Electronics SSD 960 NVMe PCIe SSD Controller ----------------------

 [General Information]
  Device Name:                            Samsung Electronics SSD 960 NVMe PCIe SSD Controller
  Original Device Name:                   Samsung Electronics SSD 960 NVMe PCIe SSD Controller
  Device Class:                           NVMe Controller
  Revision ID:                            0
  PCI Address (Bus:Device:Function) Number: 2:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_144D&DEV_A804&SUBSYS_A801144D&REV_00
 [PCI Express]
  Version:                                3.0
  Maximum Link Width:                     4x
  Current Link Width:                     4x
  Maximum Link Speed:                     8.0 GT/s
  Current Link Speed:                     8.0 GT/s
  Device/Port Type:                       PCI Express Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       >4 us
  L1 Exit Latency:                        32 - 64 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
  Memory Base Address 0                   FBE00000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    Standard NVM Express Controller
  Driver Description:                     Standard NVM Express Controller
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.527
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_144D&DEV_A804&SUBSYS_A801144D&REV_00\4&712265C&0&0009
  Location Paths                          PCIROOT(0)#PCI(0101)#PCI(0000)

Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 3a (IOU1) --------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 3a (IOU1)
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - PCI Express Root Port 3a (IOU1)
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:3:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F08&SUBSYS_0000383F&REV_02
 [PCI Express]
  Version:                                3.0
  Maximum Link Width:                     16x
  Current Link Width:                     16x
  Maximum Link Speed:                     8.0 GT/s
  Current Link Speed:                     8.0 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       Yes
  Hot-Plug:                               Not Capable
  Hot-Plug Surprise:                      Not Capable
  Slot Power Limit:                       26.000 W
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        8 - 16 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Root Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F08&SUBSYS_00008086&REV_02\3&11583659&0&18
  Location Paths                          PCIROOT(0)#PCI(0300)

PCI Express x16 Bus #3 ----------------------------------------------------


ATI/AMD Navi - Switch Upstream in PCIe ------------------------------------

 [General Information]
  Device Name:                            ATI/AMD Navi - Switch Upstream in PCIe
  Original Device Name:                   ATI/AMD Navi - Switch Upstream in PCIe
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            CA
  PCI Address (Bus:Device:Function) Number: 3:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_1002&DEV_1478&SUBSYS_0000383F&REV_CA
 [PCI Express]
  Version:                                4.0
  Maximum Link Width:                     16x
  Current Link Width:                     16x
  Maximum Link Speed:                     16.0 GT/s
  Current Link Speed:                     8.0 GT/s
  Device/Port Type:                       Upstream Port of PCI Express Switch
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        32 - 64 us
  Maximum Payload Size Supported:         512 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
  Memory Base Address 0                   FBC00000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Upstream Switch Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_1002&DEV_1478&SUBSYS_00000000&REV_CA\4&31024D2F&0&0018
  Location Paths                          PCIROOT(0)#PCI(0300)#PCI(0000)

PCI Express x16 Bus #4 ----------------------------------------------------


ATI/AMD Navi - Switch Downstream in NBIF ----------------------------------

 [General Information]
  Device Name:                            ATI/AMD Navi - Switch Downstream in NBIF
  Original Device Name:                   ATI/AMD Navi - Switch Downstream in NBIF
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            0
  PCI Address (Bus:Device:Function) Number: 4:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_1002&DEV_1479&SUBSYS_0000383F&REV_00
 [PCI Express]
  Version:                                4.0
  Maximum Link Width:                     16x
  Current Link Width:                     16x
  Maximum Link Speed:                     16.0 GT/s
  Current Link Speed:                     16.0 GT/s
  Device/Port Type:                       Downstream Port of PCI Express Switch
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         512 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Downstream Switch Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_1002&DEV_1479&SUBSYS_14791002&REV_00\5&DF6FA70&0&000018
  Location Paths                          PCIROOT(0)#PCI(0300)#PCI(0000)#PCI(0000)

PCI Express x16 Bus #5 ----------------------------------------------------


GIGABYTE RX 5600 XT WINDFORCE OC (GV-R56XTWF2OC-6GD) ----------------------

 [General Information]
  Device Name:                            GIGABYTE RX 5600 XT WINDFORCE OC (GV-R56XTWF2OC-6GD)
  Original Device Name:                   ATI/AMD Radeon RX 5600 XT (Navi 10 XLE)
  Device Class:                           VGA Compatible Adapter
  Revision ID:                            CA
  PCI Address (Bus:Device:Function) Number: 5:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_1002&DEV_731F&SUBSYS_231D1458&REV_CA
 [PCI Express]
  Version:                                4.0
  Maximum Link Width:                     16x
  Current Link Width:                     16x
  Maximum Link Speed:                     16.0 GT/s
  Current Link Speed:                     16.0 GT/s
  Device/Port Type:                       Legacy PCI Express Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Supported
  Resizable BAR0 Supported Size:          256 MB, 512 MB, 1 GB
  Resizable BAR0 Current Size:            256 MB
  Resizable BAR1 Supported Size:          2 MB, 4 MB, 8 MB, 16 MB, 32 MB, 64 MB, 128 MB, 256 MB
  Resizable BAR1 Current Size:            2 MB
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
  Memory Base Address 0                   383FE0000000
  Memory Base Address 2                   383FF0000000
  I/O Base Address 4                      FF00
  Memory Base Address 5                   FBB00000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    Advanced Micro Devices, Inc.
  Driver Description:                     AMD Radeon RX 5600 XT
  Driver Provider:                        Advanced Micro Devices, Inc.
  Driver Version:                         30.0.21017.1000
  AMD Driver Package Version:             22.10.17.01-220517a-379774C-AMD-Software-Adrenalin-Edition
  AMD Software Driver Version:            22.5.2
  Driver Date:                            16-May-2022
  DCH/UWD Driver:                         Capable
  DeviceInstanceId                        PCI\VEN_1002&DEV_731F&SUBSYS_231D1458&REV_CA\6&2A0AE5FB&0&00000018
  Location Paths                          PCIROOT(0)#PCI(0300)#PCI(0000)#PCI(0000)#PCI(0000)

ATI/AMD Navi1x - High Definition Audio Controller -------------------------

 [General Information]
  Device Name:                            ATI/AMD Navi1x - High Definition Audio Controller
  Original Device Name:                   ATI/AMD Navi1x - High Definition Audio Controller
  Device Class:                           High Definition Audio
  Revision ID:                            0
  PCI Address (Bus:Device:Function) Number: 5:0:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_1002&DEV_AB38&SUBSYS_AB381002&REV_00
 [PCI Express]
  Version:                                4.0
  Maximum Link Width:                     16x
  Current Link Width:                     16x
  Maximum Link Speed:                     16.0 GT/s
  Current Link Speed:                     16.0 GT/s
  Device/Port Type:                       Legacy PCI Express Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         256 bytes
  Maximum Payload Size:                   256 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         IRQ44
  Interrupt Pin:                          INTB#
  Memory Base Address 0                   FBBFC000
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    AMD
  Driver Description:                     High Definition Audio Bus
  Driver Provider:                        AMD
  Driver Version:                         21.30.0.1000
  Driver Date:                            16-Sep-2021
  DeviceInstanceId                        PCI\VEN_1002&DEV_AB38&SUBSYS_AB381002&REV_00\6&2A0AE5FB&0&01000018
  Location Paths                          PCIROOT(0)#PCI(0300)#PCI(0000)#PCI(0000)#PCI(0001)

Intel Haswell-EN/EP/EP 4S/EX IIO - VT, Address Map, System Management, Miscellaneous

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - VT, Address Map, System Management, Miscellaneous
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - VT, Address Map, System Management, Miscellaneous
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:5:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F28&SUBSYS_00008086&REV_02
 [PCI Express]
  Version:                                2.0
  Current Link Width:                     Not negotiated
  Maximum Link Speed:                     5.0 GT/s
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: None
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F28&SUBSYS_00008086&REV_02\3&11583659&0&28
  Location Paths                          PCIROOT(0)#PCI(0500)

Intel Haswell-EN/EP/EP 4S/EX IIO - Hot Plug -------------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - Hot Plug
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - Hot Plug
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:5:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F29&SUBSYS_00008086&REV_02
 [PCI Express]
  Version:                                1.1
  Current Link Width:                     Not negotiated
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: None
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F29&SUBSYS_00008086&REV_02\3&11583659&0&29
  Location Paths                          PCIROOT(0)#PCI(0501)

Intel Haswell-EN/EP/EP 4S/EX IIO - RAS, Control Status and Global Errors --

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - RAS, Control Status and Global Errors
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - RAS, Control Status and Global Errors
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:5:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F2A&SUBSYS_00008086&REV_02
 [PCI Express]
  Version:                                2.0
  Current Link Width:                     Not negotiated
  Maximum Link Speed:                     5.0 GT/s
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: None
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F2A&SUBSYS_00008086&REV_02\3&11583659&0&2A
  Location Paths                          PCIROOT(0)#PCI(0502)

Intel Haswell-EN/EP/EP 4S/EX IIO - I/OxAPIC -------------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX IIO - I/OxAPIC
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX IIO - I/OxAPIC
  Device Class:                           I/O(X) APIC
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 0:5:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F2C&SUBSYS_00008086&REV_02
 [PCI Express]
  Version:                                1.1
  Current Link Width:                     Not negotiated
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: None
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
  Memory Base Address 0                   FBF02000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F2C&SUBSYS_00008086&REV_02\3&11583659&0&2C
  Location Paths                          PCIROOT(0)#PCI(0504)

Intel Wellsburg PCH - Server Platform Services ROM (SPSR) [B1] ------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - Server Platform Services ROM (SPSR) [B1]
  Original Device Name:                   Intel Wellsburg PCH - Server Platform Services ROM (SPSR) [B1]
  Device Class:                           Unknown
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:17:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D7C&SUBSYS_72708086&REV_05
 [PCI Express]
  Version:                                2.0
  Maximum Link Width:                     1x
  Current Link Width:                     1x
  Maximum Link Speed:                     5.0 GT/s
  Current Link Speed:                     2.5 GT/s
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D7C&SUBSYS_72708086&REV_05\3&11583659&0&88
  Location Paths                          PCIROOT(0)#PCI(1100)

Intel Wellsburg PCH - USB 3.0 xHCI Host Controller [B1] -------------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - USB 3.0 xHCI Host Controller [B1]
  Original Device Name:                   Intel Wellsburg PCH - USB 3.0 xHCI Host Controller [B1]
  Device Class:                           USB xHCI Controller
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:20:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D31&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         IRQ19
  Interrupt Pin:                          INTD#
  Memory Base Address 0                   383FFFF00000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Capable
  USB Version Supported:                  3.0
 [Driver Information]
  Driver Manufacturer:                    Generic USB xHCI Host Controller
  Driver Description:                     USB xHCI Compliant Host Controller
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            11-May-2022
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D31&SUBSYS_72708086&REV_05\3&11583659&0&A0
  Location Paths                          PCIROOT(0)#PCI(1400)

USB Root Hub --------------------------------------------------------------


[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : Realtek Semiconductor 4-Port USB 3 Hub --------------------------

 [Device Information]
  Device Manufacturer:                    Generic
  Product Name:                           4-Port USB 2.0 Hub
  Serial Number:                          N/A
  USB Version Supported:                  3.00 (Connected to a USB 2.00 Port)
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_0BDA&PID_5411
 [Driver Information]
  Driver Manufacturer:                    (Standard USB HUBs)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.65
  Driver Date:                            02-Jul-2021
  DeviceInstanceId                        USB\VID_0BDA&PID_5411\5&1932DDEF&0&6
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(6)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : Holtek Microelectronics, PID=FC02 -------------------------------

 [Device Information]
  Device Manufacturer:                    OBINS
  Product Name:                           OBINS
AnnePro2
  Serial Number:                          00000000000000000000000000000000
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 1.1 Full-speed
  Driver Description:                     USB Composite Device
  Hardware ID:                            USB\VID_04D9&PID_A293
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     USB Composite Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_04D9&PID_A293\00000000000000000000000000000000
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(6)#USB(4)

[Port7] : No Device Connected ---------------------------------------------


[Port8] : No Device Connected ---------------------------------------------


[Port9] : No Device Connected ---------------------------------------------


[Port10] : No Device Connected --------------------------------------------


[Port11] : No Device Connected --------------------------------------------


[Port12] : No Device Connected --------------------------------------------


[Port13] : No Device Connected --------------------------------------------


[Port14] : Logitech Cordless Mouse ----------------------------------------

 [Device Information]
  Device Manufacturer:                    Logitech
  Product Name:                           USB Receiver
  Serial Number:                          N/A
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 1.1 Full-speed
  Driver Description:                     USB Composite Device
  Hardware ID:                            USB\VID_046D&PID_C52F
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     USB Composite Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_046D&PID_C52F\5&1932DDEF&0&14
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(14)

[Port15] : No Device Connected --------------------------------------------


[Port16] : No Device Connected --------------------------------------------


[Port17] : SanDisk Ultra Flair --------------------------------------------

 [Device Information]
  Device Manufacturer:                    SanDisk
  Product Name:                           Ultra USB 3.0
  Serial Number:                          04014b313b1ab4c951b133dec56456ad315c981acc6dff524ddfdfc4abf95501586a00000000000000000000cc104d700015081891558107b3a7208b
  USB Version Supported:                  3.00
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     USB Mass Storage Device
  Hardware ID:                            USB\VID_0781&PID_5591
 [Driver Information]
  Driver Manufacturer:                    Compatible USB storage device
  Driver Description:                     USB Mass Storage Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.653
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_0781&PID_5591\04014B313B1AB4C951B133DEC56456AD315C981ACC6DFF524DDFDFC4ABF95501586A00000000000000000000CC104D700015081891558107B3A7208B
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(17)

[Port18] : Realtek Semiconductor, PID=F192 --------------------------------

 [Device Information]
  Device Manufacturer:                    Sabrent
  Product Name:                           Sabrent
  Serial Number:                          012345678930
  USB Version Supported:                  3.20
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     USB Attached SCSI (UAS) Mass Storage Device
  Hardware ID:                            USB\VID_0BDA&PID_9210
 [Driver Information]
  Driver Manufacturer:                    USB Attached SCSI (UAS) Compatible Device
  Driver Description:                     USB Attached SCSI (UAS) Mass Storage Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.653
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_0BDA&PID_9210\MSFT30012345678930
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(18)

[Port19] : Realtek Semiconductor 4-Port USB 3 Hub -------------------------

 [Device Information]
  Device Manufacturer:                    Realtek Semiconductor
  Product Name:                           Realtek Semiconductor 4-Port USB 3 Hub
  Serial Number:                          -
  USB Version Supported:                  3.00
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     Generic SuperSpeed USB Hub
  Hardware ID:                            USB\VID_0BDA&PID_0411
 [Driver Information]
  Driver Manufacturer:                    (Standard USB HUBs)
  Driver Description:                     Generic SuperSpeed USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.65
  Driver Date:                            02-Jul-2021
  DeviceInstanceId                        USB\VID_0BDA&PID_0411\5&1932DDEF&0&19
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(19)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port20] : No Device Connected --------------------------------------------


[Port21] : No Device Connected --------------------------------------------


Intel Wellsburg PCH - Host Embedded Controller Interface 1 (HECI1) [B1] ---

 [General Information]
  Device Name:                            Intel Wellsburg PCH - Host Embedded Controller Interface 1 (HECI1) [B1]
  Original Device Name:                   Intel Wellsburg PCH - Host Embedded Controller Interface 1 (HECI1) [B1]
  Device Class:                           Other Communication Device
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:22:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D3A&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
  Memory Base Address 0                   383FFFFFBFF0
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    Intel
  Driver Description:                     Intel(R) Management Engine Interface 
  Driver Provider:                        Intel
  Driver Version:                         11.7.0.1045
  Driver Date:                            02-Oct-2017
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D3A&SUBSYS_72708086&REV_05\3&11583659&0&B0
  Location Paths                          PCIROOT(0)#PCI(1600)

Intel Wellsburg PCH - Host Embedded Controller Interface 2 (HECI2) [B1] ---

 [General Information]
  Device Name:                            Intel Wellsburg PCH - Host Embedded Controller Interface 2 (HECI2) [B1]
  Original Device Name:                   Intel Wellsburg PCH - Host Embedded Controller Interface 2 (HECI2) [B1]
  Device Class:                           Other Communication Device
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:22:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D3B&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTB#
  Memory Base Address 0                   383FFFF16000
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D3B&SUBSYS_72708086&REV_05\3&11583659&0&B1
  Location Paths                          PCIROOT(0)#PCI(1601)

Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #2 [B1] ----------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #2 [B1]
  Original Device Name:                   Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #2 [B1]
  Device Class:                           USB EHCI Controller
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:26:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D2D&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         IRQ18
  Interrupt Pin:                          INTC#
  Memory Base Address 0                   FBF01000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Capable
  USB Version Supported:                  2.0
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     Standard Enhanced PCI to USB Host Controller
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D2D&SUBSYS_72708086&REV_05\3&11583659&0&D0
  Location Paths                          PCIROOT(0)#PCI(1A00)

USB Root Hub --------------------------------------------------------------


[Port1] : Intel Integrated Rate Matching Hub ------------------------------

 [Device Information]
  Device Manufacturer:                    Intel
  Product Name:                           Intel Integrated Rate Matching Hub
  Serial Number:                          
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_8087&PID_800A
 [Driver Information]
  Driver Manufacturer:                    (Generic USB Hub)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_8087&PID_800A\5&117D1CCD&0&1
  Location Paths                          PCIROOT(0)#PCI(1A00)#USBROOT(0)#USB(1)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


Intel Wellsburg PCH - High Definition Audio Controller [B1] ---------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - High Definition Audio Controller [B1]
  Original Device Name:                   Intel Wellsburg PCH - High Definition Audio Controller [B1]
  Device Class:                           High Definition Audio
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:27:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D20&SUBSYS_72708086&REV_05
 [PCI Express]
  Version:                                1.1
  Current Link Width:                     Not negotiated
  Device/Port Type:                       Root Complex Integrated Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: None
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       < 64 ns
  L1 Exit Latency:                        < 1 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         IRQ22
  Interrupt Pin:                          INTA#
  Memory Base Address 0                   383FFFFFC000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    Microsoft
  Driver Description:                     High Definition Audio Controller
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            04-Jun-2021
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D20&SUBSYS_72708086&REV_05\3&11583659&0&D8
  Location Paths                          PCIROOT(0)#PCI(1B00)

Intel Wellsburg PCH - PCI Express Root Port 1 [B1] ------------------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - PCI Express Root Port 1 [B1]
  Original Device Name:                   Intel Wellsburg PCH - PCI Express Root Port 1 [B1]
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            D5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:28:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D10&SUBSYS_00000000&REV_D5
 [PCI Express]
  Version:                                2.0
  Maximum Link Width:                     1x
  Current Link Width:                     Not negotiated
  Maximum Link Speed:                     5.0 GT/s
  Current Link Speed:                     2.5 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       512 ns - 1 us
  L1 Exit Latency:                        2 - 4 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Root Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D10&SUBSYS_72708086&REV_D5\3&11583659&0&E0
  Location Paths                          PCIROOT(0)#PCI(1C00)

PCI Express x1 Bus #6 -----------------------------------------------------


Intel Wellsburg PCH - PCI Express Root Port 8 [B1] ------------------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - PCI Express Root Port 8 [B1]
  Original Device Name:                   Intel Wellsburg PCH - PCI Express Root Port 8 [B1]
  Device Class:                           PCI-to-PCI Bridge
  Revision ID:                            D5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:28:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D1E&SUBSYS_0000383F&REV_D5
 [PCI Express]
  Version:                                2.0
  Maximum Link Width:                     1x
  Current Link Width:                     1x
  Maximum Link Speed:                     5.0 GT/s
  Current Link Speed:                     2.5 GT/s
  Device/Port Type:                       Root Port of PCI Express Root Complex
  Slot Implemented:                       Yes
  Hot-Plug:                               Not Capable
  Hot-Plug Surprise:                      Not Capable
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: L1 Entry
  L0s Exit Latency:                       256 - 512 ns
  L1 Exit Latency:                        2 - 4 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTD#
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI Express Root Port
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D1E&SUBSYS_72708086&REV_D5\3&11583659&0&E7
  Location Paths                          PCIROOT(0)#PCI(1C07)

PCI Express x1 Bus #7 -----------------------------------------------------


RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC -------------

 [General Information]
  Device Name:                            RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC
  Original Device Name:                   RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC
  Device Class:                           Ethernet Adapter
  Revision ID:                            9
  PCI Address (Bus:Device:Function) Number: 7:0:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_10EC&DEV_8168&SUBSYS_012310EC&REV_09
 [PCI Express]
  Version:                                2.0
  Maximum Link Width:                     1x
  Current Link Width:                     1x
  Maximum Link Speed:                     5.0 GT/s
  Current Link Speed:                     2.5 GT/s
  Device/Port Type:                       PCI Express Endpoint
  Slot Implemented:                       No
  Emergency Power Reduction:              Not Supported
  Active State Power Management (ASPM) Support: L0s and L1
  Active State Power Management (ASPM) Status: Disabled
  L0s Exit Latency:                       >4 us
  L1 Exit Latency:                        32 - 64 us
  Maximum Payload Size Supported:         128 bytes
  Maximum Payload Size:                   128 bytes
  Resizable BAR Support:                  Not Supported
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTA#
  I/O Base Address 0                      E000
  Memory Base Address 2                   FBD00000
  Memory Base Address 4                   383FF0300000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    Realtek
  Driver Description:                     Realtek PCIe GbE Family Controller
  Driver Provider:                        Microsoft
  Driver Version:                         9.1.411.2015
  Driver Date:                            10-Apr-2015
  DeviceInstanceId                        PCI\VEN_10EC&DEV_8168&SUBSYS_012310EC&REV_09\78000000684CE00000
  Location Paths                          PCIROOT(0)#PCI(1C07)#PCI(0000)

Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #1 [B1] ----------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #1 [B1]
  Original Device Name:                   Intel Wellsburg PCH - USB 2.0 EHCI Host Controller #1 [B1]
  Device Class:                           USB EHCI Controller
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:29:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D26&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         IRQ18
  Interrupt Pin:                          INTC#
  Memory Base Address 0                   FBF00000
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Capable
  USB Version Supported:                  2.0
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     Standard Enhanced PCI to USB Host Controller
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.708
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D26&SUBSYS_72708086&REV_05\3&11583659&0&E8
  Location Paths                          PCIROOT(0)#PCI(1D00)

USB Root Hub --------------------------------------------------------------


[Port1] : Intel Integrated Rate Matching Hub ------------------------------

 [Device Information]
  Device Manufacturer:                    Intel
  Product Name:                           Intel Integrated Rate Matching Hub
  Serial Number:                          
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_8087&PID_8002
 [Driver Information]
  Driver Manufacturer:                    (Generic USB Hub)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_8087&PID_8002\5&12B5DBAE&0&1
  Location Paths                          PCIROOT(0)#PCI(1D00)#USBROOT(0)#USB(1)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : No Device Connected ---------------------------------------------


[Port7] : No Device Connected ---------------------------------------------


[Port8] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


Intel Wellsburg-G - LPC Interface Controller [B1] -------------------------

 [General Information]
  Device Name:                            Intel Wellsburg-G - LPC Interface Controller [B1]
  Original Device Name:                   Intel Wellsburg-G - LPC Interface Controller [B1]
  Device Class:                           PCI-to-ISA Bridge
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:31:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D44&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Enabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
 [Driver Information]
  Driver Manufacturer:                    (Standard system devices)
  Driver Description:                     PCI standard ISA bridge
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D44&SUBSYS_72708086&REV_05\3&11583659&0&F8
  Location Paths                          PCIROOT(0)#PCI(1F00)

Intel Wellsburg PCH - SMBus Controller [B1] -------------------------------

 [General Information]
  Device Name:                            Intel Wellsburg PCH - SMBus Controller [B1]
  Original Device Name:                   Intel Wellsburg PCH - SMBus Controller [B1]
  Device Class:                           SMBus (System Management Bus)
  Revision ID:                            5 [B1]
  PCI Address (Bus:Device:Function) Number: 0:31:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_8D22&SUBSYS_72708086&REV_05
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          INTC#
  Memory Base Address 0                   383FFFF15000
  I/O Base Address 4                      580
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_8D22&SUBSYS_72708086&REV_05\3&11583659&0&FB
  Location Paths                          PCIROOT(0)#PCI(1F03)

PCI Bus #255 --------------------------------------------------------------


Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:11:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F81&SUBSYS_2F818086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F81&SUBSYS_2F818086&REV_02\3&103A9D54&0&58
  Location Paths                          PCIROOT(FF)#PCI(0B00)

Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:11:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F36&SUBSYS_2F368086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F36&SUBSYS_2F368086&REV_02\3&103A9D54&0&59
  Location Paths                          PCIROOT(FF)#PCI(0B01)

Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - R3 Intel QPI Link 0 & 1 Performance Monitoring
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:11:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F37&SUBSYS_2F378086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F37&SUBSYS_2F378086&REV_02\3&103A9D54&0&5A
  Location Paths                          PCIROOT(FF)#PCI(0B02)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE0&SUBSYS_2FE08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE0&SUBSYS_2FE08086&REV_02\3&103A9D54&0&60
  Location Paths                          PCIROOT(FF)#PCI(0C00)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE1&SUBSYS_2FE18086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE1&SUBSYS_2FE18086&REV_02\3&103A9D54&0&61
  Location Paths                          PCIROOT(FF)#PCI(0C01)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE2&SUBSYS_2FE28086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE2&SUBSYS_2FE28086&REV_02\3&103A9D54&0&62
  Location Paths                          PCIROOT(FF)#PCI(0C02)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE3&SUBSYS_2FE38086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE3&SUBSYS_2FE38086&REV_02\3&103A9D54&0&63
  Location Paths                          PCIROOT(FF)#PCI(0C03)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE4&SUBSYS_2FE48086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE4&SUBSYS_2FE48086&REV_02\3&103A9D54&0&64
  Location Paths                          PCIROOT(FF)#PCI(0C04)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE5&SUBSYS_2FE58086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE5&SUBSYS_2FE58086&REV_02\3&103A9D54&0&65
  Location Paths                          PCIROOT(FF)#PCI(0C05)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE6&SUBSYS_2FE68086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE6&SUBSYS_2FE68086&REV_02\3&103A9D54&0&66
  Location Paths                          PCIROOT(FF)#PCI(0C06)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:12:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE7&SUBSYS_2FE78086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE7&SUBSYS_2FE78086&REV_02\3&103A9D54&0&67
  Location Paths                          PCIROOT(FF)#PCI(0C07)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE8&SUBSYS_2FE88086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE8&SUBSYS_2FE88086&REV_02\3&103A9D54&0&68
  Location Paths                          PCIROOT(FF)#PCI(0D00)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FE9&SUBSYS_2FE98086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FE9&SUBSYS_2FE98086&REV_02\3&103A9D54&0&69
  Location Paths                          PCIROOT(FF)#PCI(0D01)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FEA&SUBSYS_2FEA8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FEA&SUBSYS_2FEA8086&REV_02\3&103A9D54&0&6A
  Location Paths                          PCIROOT(FF)#PCI(0D02)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FEB&SUBSYS_2FEB8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FEB&SUBSYS_2FEB8086&REV_02\3&103A9D54&0&6B
  Location Paths                          PCIROOT(FF)#PCI(0D03)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FEC&SUBSYS_2FEC8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FEC&SUBSYS_2FEC8086&REV_02\3&103A9D54&0&6C
  Location Paths                          PCIROOT(FF)#PCI(0D04)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FED&SUBSYS_2FED8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FED&SUBSYS_2FED8086&REV_02\3&103A9D54&0&6D
  Location Paths                          PCIROOT(FF)#PCI(0D05)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FEE&SUBSYS_2FEE8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FEE&SUBSYS_2FEE8086&REV_02\3&103A9D54&0&6E
  Location Paths                          PCIROOT(FF)#PCI(0D06)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:13:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FEF&SUBSYS_2FEF8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FEF&SUBSYS_2FEF8086&REV_02\3&103A9D54&0&6F
  Location Paths                          PCIROOT(FF)#PCI(0D07)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:14:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FF0&SUBSYS_2FF08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FF0&SUBSYS_2FF08086&REV_02\3&103A9D54&0&70
  Location Paths                          PCIROOT(FF)#PCI(0E00)

Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers ----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX CBo - Unicast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:14:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FF1&SUBSYS_2FF18086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FF1&SUBSYS_2FF18086&REV_02\3&103A9D54&0&71
  Location Paths                          PCIROOT(FF)#PCI(0E01)

Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents -

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FF8&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FF8&SUBSYS_00000000&REV_02\3&103A9D54&0&78
  Location Paths                          PCIROOT(FF)#PCI(0F00)

Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents -

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FF9&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FF9&SUBSYS_00000000&REV_02\3&103A9D54&0&79
  Location Paths                          PCIROOT(FF)#PCI(0F01)

Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents -

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FFA&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FFA&SUBSYS_00000000&REV_02\3&103A9D54&0&7A
  Location Paths                          PCIROOT(FF)#PCI(0F02)

Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents -

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Caching Agent (Cbo) - Buffered Ring Agents
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FFB&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FFB&SUBSYS_00000000&REV_02\3&103A9D54&0&7B
  Location Paths                          PCIROOT(FF)#PCI(0F03)

Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FFC&SUBSYS_2FE08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FFC&SUBSYS_2FE08086&REV_02\3&103A9D54&0&7C
  Location Paths                          PCIROOT(FF)#PCI(0F04)

Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FFD&SUBSYS_2FE08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FFD&SUBSYS_2FE08086&REV_02\3&103A9D54&0&7D
  Location Paths                          PCIROOT(FF)#PCI(0F05)

Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Cbo System Address Decoder and Broadcast Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:15:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FFE&SUBSYS_2FE08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FFE&SUBSYS_2FE08086&REV_02\3&103A9D54&0&7E
  Location Paths                          PCIROOT(FF)#PCI(0F06)

Intel Haswell-EN/EP/EP 4S/EX - R2PCIE -------------------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - R2PCIE
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - R2PCIE
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:16:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F1D&SUBSYS_2F1D8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F1D&SUBSYS_2F1D8086&REV_02\3&103A9D54&0&80
  Location Paths                          PCIROOT(FF)#PCI(1000)

Intel Haswell-EN/EP/EP 4S/EX - R2PCIE -------------------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - R2PCIE
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - R2PCIE
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:16:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F34&SUBSYS_2F348086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F34&SUBSYS_2F348086&REV_02\3&103A9D54&0&81
  Location Paths                          PCIROOT(FF)#PCI(1001)

Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores -------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:16:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F1E&SUBSYS_2F1E8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F1E&SUBSYS_2F1E8086&REV_02\3&103A9D54&0&85
  Location Paths                          PCIROOT(FF)#PCI(1005)

Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores -------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:16:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F7D&SUBSYS_2F7D8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F7D&SUBSYS_2F7D8086&REV_02\3&103A9D54&0&86
  Location Paths                          PCIROOT(FF)#PCI(1006)

Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores -------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX UBox - Scratchpad and Semaphores
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:16:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F1F&SUBSYS_2F1F8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F1F&SUBSYS_2F1F8086&REV_02\3&103A9D54&0&87
  Location Paths                          PCIROOT(FF)#PCI(1007)

Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 - TAD and HA Config -----------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 - TAD and HA Config
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 - TAD and HA Config
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:18:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FA0&SUBSYS_2FA08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FA0&SUBSYS_2FA08086&REV_02\3&103A9D54&0&90
  Location Paths                          PCIROOT(FF)#PCI(1200)

Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 Perfmon -----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 Perfmon
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Home Agent 0 Perfmon
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:18:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F30&SUBSYS_2F308086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F30&SUBSYS_2F308086&REV_02\3&103A9D54&0&91
  Location Paths                          PCIROOT(FF)#PCI(1201)

Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 - TAD and HA Config -----------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 - TAD and HA Config
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 - TAD and HA Config
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:18:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F60&SUBSYS_2F608086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F60&SUBSYS_2F608086&REV_02\3&103A9D54&0&94
  Location Paths                          PCIROOT(FF)#PCI(1204)

Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 Perfmon -----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 Perfmon
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Home Agent 1 Perfmon
  Device Class:                           Performance counters
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:18:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F38&SUBSYS_2F388086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F38&SUBSYS_2F388086&REV_02\3&103A9D54&0&95
  Location Paths                          PCIROOT(FF)#PCI(1205)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FA8&SUBSYS_2FA88086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FA8&SUBSYS_2FA88086&REV_02\3&103A9D54&0&98
  Location Paths                          PCIROOT(FF)#PCI(1300)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Target Address / Thermal / RAS
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F71&SUBSYS_2F718086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F71&SUBSYS_2F718086&REV_02\3&103A9D54&0&99
  Location Paths                          PCIROOT(FF)#PCI(1301)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FAA&SUBSYS_2FAA8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FAA&SUBSYS_2FAA8086&REV_02\3&103A9D54&0&9A
  Location Paths                          PCIROOT(FF)#PCI(1302)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel Target Address Decoder Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FAB&SUBSYS_2FAB8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FAB&SUBSYS_2FAB8086&REV_02\3&103A9D54&0&9B
  Location Paths                          PCIROOT(FF)#PCI(1303)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Channel 0/1 Broadcast

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Channel 0/1 Broadcast
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Channel 0/1 Broadcast
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FAE&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FAE&SUBSYS_00000000&REV_02\3&103A9D54&0&9E
  Location Paths                          PCIROOT(FF)#PCI(1306)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Global Broadcast

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Global Broadcast
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - DDRIO Global Broadcast
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:19:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FAF&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FAF&SUBSYS_00000000&REV_02\3&103A9D54&0&9F
  Location Paths                          PCIROOT(FF)#PCI(1307)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 Thermal Control

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 Thermal Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 Thermal Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB0&SUBSYS_2FB08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB0&SUBSYS_2FB08086&REV_02\3&103A9D54&0&A0
  Location Paths                          PCIROOT(FF)#PCI(1400)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 Thermal Control

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 Thermal Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 Thermal Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB1&SUBSYS_2FB18086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB1&SUBSYS_2FB18086&REV_02\3&103A9D54&0&A1
  Location Paths                          PCIROOT(FF)#PCI(1401)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 ERROR Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 ERROR Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 0 ERROR Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB2&SUBSYS_2FB28086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB2&SUBSYS_2FB28086&REV_02\3&103A9D54&0&A2
  Location Paths                          PCIROOT(FF)#PCI(1402)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 ERROR Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 ERROR Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 0 - Channel 1 ERROR Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB3&SUBSYS_2FB38086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB3&SUBSYS_2FB38086&REV_02\3&103A9D54&0&A3
  Location Paths                          PCIROOT(FF)#PCI(1403)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Normal Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Normal Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Normal Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBC&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBC&SUBSYS_00000000&REV_02\3&103A9D54&0&A4
  Location Paths                          PCIROOT(FF)#PCI(1404)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Extended Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Extended Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE0 Extended Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBD&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBD&SUBSYS_00000000&REV_02\3&103A9D54&0&A5
  Location Paths                          PCIROOT(FF)#PCI(1405)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Normal Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Normal Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Normal Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBE&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBE&SUBSYS_00000000&REV_02\3&103A9D54&0&A6
  Location Paths                          PCIROOT(FF)#PCI(1406)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Extended Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Extended Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE1 Extended Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:20:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBF&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBF&SUBSYS_00000000&REV_02\3&103A9D54&0&A7
  Location Paths                          PCIROOT(FF)#PCI(1407)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F68&SUBSYS_2F688086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F68&SUBSYS_2F688086&REV_02\3&103A9D54&0&B0
  Location Paths                          PCIROOT(FF)#PCI(1600)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Target Address / Thermal / RAS
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F79&SUBSYS_2F798086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F79&SUBSYS_2F798086&REV_02\3&103A9D54&0&B1
  Location Paths                          PCIROOT(FF)#PCI(1601)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F6A&SUBSYS_2F6A8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F6A&SUBSYS_2F6A8086&REV_02\3&103A9D54&0&B2
  Location Paths                          PCIROOT(FF)#PCI(1602)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel Target Address Decoder Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F6B&SUBSYS_2F6B8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F6B&SUBSYS_2F6B8086&REV_02\3&103A9D54&0&B3
  Location Paths                          PCIROOT(FF)#PCI(1603)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Channel 2/3 Broadcast

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Channel 2/3 Broadcast
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Channel 2/3 Broadcast
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F6E&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F6E&SUBSYS_00000000&REV_02\3&103A9D54&0&B6
  Location Paths                          PCIROOT(FF)#PCI(1606)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Global Broadcast

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Global Broadcast
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - DDRIO Global Broadcast
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:22:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F6F&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F6F&SUBSYS_00000000&REV_02\3&103A9D54&0&B7
  Location Paths                          PCIROOT(FF)#PCI(1607)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0 Thermal Control

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0 Thermal Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0 Thermal Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FD0&SUBSYS_2FD08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FD0&SUBSYS_2FD08086&REV_02\3&103A9D54&0&B8
  Location Paths                          PCIROOT(FF)#PCI(1700)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 1 Thermal Control

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 1 Thermal Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 1 Thermal Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FD1&SUBSYS_2FD18086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FD1&SUBSYS_2FD18086&REV_02\3&103A9D54&0&B9
  Location Paths                          PCIROOT(FF)#PCI(1701)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FD2&SUBSYS_2FD28086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FD2&SUBSYS_2FD28086&REV_02\3&103A9D54&0&BA
  Location Paths                          PCIROOT(FF)#PCI(1702)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller 1 - Channel 0-3 ERROR Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FD3&SUBSYS_2FD38086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FD3&SUBSYS_2FD38086&REV_02\3&103A9D54&0&BB
  Location Paths                          PCIROOT(FF)#PCI(1703)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Normal Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Normal Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Normal Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB8&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB8&SUBSYS_00000000&REV_02\3&103A9D54&0&BC
  Location Paths                          PCIROOT(FF)#PCI(1704)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Extended Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Extended Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE2 Extended Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:5
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FB9&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FB9&SUBSYS_00000000&REV_02\3&103A9D54&0&BD
  Location Paths                          PCIROOT(FF)#PCI(1705)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Normal Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Normal Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Normal Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:6
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBA&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBA&SUBSYS_00000000&REV_02\3&103A9D54&0&BE
  Location Paths                          PCIROOT(FF)#PCI(1706)

Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Extended Registers

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Extended Registers
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Integrated Memory Controller DDRIO - VMSE3 Extended Registers
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:23:7
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FBB&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FBB&SUBSYS_00000000&REV_02\3&103A9D54&0&BF
  Location Paths                          PCIROOT(FF)#PCI(1707)

Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control ---------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:30:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F98&SUBSYS_2F988086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F98&SUBSYS_2F988086&REV_02\3&103A9D54&0&F0
  Location Paths                          PCIROOT(FF)#PCI(1E00)

Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control ---------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:30:1
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F99&SUBSYS_2F998086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F99&SUBSYS_2F998086&REV_02\3&103A9D54&0&F1
  Location Paths                          PCIROOT(FF)#PCI(1E01)

Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control ---------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:30:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F9A&SUBSYS_2F9A8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F9A&SUBSYS_2F9A8086&REV_02\3&103A9D54&0&F2
  Location Paths                          PCIROOT(FF)#PCI(1E02)

Intel Haswell-EN/EP/EP 4S/EX - Power Control Unit 0 -----------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Control Unit 0
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Control Unit 0
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:30:3
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2FC0&SUBSYS_2FC08086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
  I/O Base Address 0                      14
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2FC0&SUBSYS_2FC08086&REV_02\3&103A9D54&0&F3
  Location Paths                          PCIROOT(FF)#PCI(1E03)

Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control ---------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:30:4
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F9C&SUBSYS_2F9C8086&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F9C&SUBSYS_2F9C8086&REV_02\3&103A9D54&0&F4
  Location Paths                          PCIROOT(FF)#PCI(1E04)

Intel Haswell-EN/EP/EP 4S/EX - VCU ----------------------------------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - VCU
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - VCU
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:31:0
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F88&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F88&SUBSYS_00000000&REV_02\3&103A9D54&0&F8
  Location Paths                          PCIROOT(FF)#PCI(1F00)

Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control ---------------

 [General Information]
  Device Name:                            Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Original Device Name:                   Intel Haswell-EN/EP/EP 4S/EX - Power Management and Control
  Device Class:                           Unknown Peripheral Device
  Revision ID:                            2
  PCI Address (Bus:Device:Function) Number: 255:31:2
  PCI Latency Timer:                      0
  Hardware ID:                            PCI\VEN_8086&DEV_2F8A&SUBSYS_00000000&REV_02
 [System Resources]
  Interrupt Line:                         N/A
  Interrupt Pin:                          N/A
 [Features]
  Bus Mastering:                          Disabled
  Running At 66 MHz:                      Not Capable
  Fast Back-to-Back Transactions:         Not Capable
  DeviceInstanceId                        PCI\VEN_8086&DEV_2F8A&SUBSYS_00000000&REV_02\3&103A9D54&0&FA
  Location Paths                          PCIROOT(FF)#PCI(1F02)

Video Adapter -------------------------------------------------------------


AMD Radeon RX 5600 XT -----------------------------------------------------

 [Video chipset]
  Video Chipset:                          AMD Radeon RX 5600 XT
  Video Chipset Codename:                 Navi10 XLE
  Video Memory:                           6128 MBytes of GDDR6 SDRAM [Micron]
 [Video Card]
  Video Card:                             GIGABYTE RX 5600 XT WINDFORCE OC (GV-R56XTWF2OC-6GD)
  Video Bus:                              PCIe v4.0 x16 (16.0 GT/s) @ x16 (8.0 GT/s)
  Video RAMDAC:                           Internal DAC(400MHz)
  Video BIOS Version:                     017.001.000.068
 [Performance]
  Graphics Processor Clock:               10.0 MHz
  Graphics Memory Clock:                  216.0 MHz (Effective 1728.0 MHz)
  Graphics Memory Bus Width:              256-bit
  Number Of ROPs:                         64
  Number Of Unified Shaders:              2304
  Number Of TMUs (Texture Mapping Units): 144
  SMU Firmware Version:                   0.42.65
  Resizable BAR (ReBAR) Support:          Supported
  Resizable BAR (ReBAR) State:            Disabled (256 MB)
  Hardware ID:                            PCI\VEN_1002&DEV_731F&SUBSYS_231D1458&REV_CA
  PCI Location (Bus:Dev:Fnc):             5:00:0
 [Driver Information]
  Driver Manufacturer:                    Advanced Micro Devices, Inc.
  Driver Description:                     AMD Radeon RX 5600 XT
  Driver Provider:                        Advanced Micro Devices, Inc.
  Driver Version:                         30.0.21017.1000
  AMD Driver Package Version:             22.10.17.01-220517a-379774C-AMD-Software-Adrenalin-Edition
  AMD Software Driver Version:            22.5.2
  Driver Date:                            16-May-2022
  DCH/UWD Driver:                         Capable
  DeviceInstanceId                        PCI\VEN_1002&DEV_731F&SUBSYS_231D1458&REV_CA\6&2A0AE5FB&0&00000018
  Location Paths                          PCIROOT(0)#PCI(0300)#PCI(0000)#PCI(0000)#PCI(0000)

Monitor -------------------------------------------------------------------


SAMSUNG [Unknown Model: SAM1016] ------------------------------------------

 [General information]
  Monitor Name:                           SAMSUNG [Unknown Model: SAM1016]
  Monitor Name (Manuf):                   LU28R55      
  Serial Number:                          Unknown
  Date Of Manufacture:                    Week: 14, Year: 2021
  Monitor Hardware ID:                    Monitor\SAM1016
  Max. Vertical Size:                     36 cm
  Max. Horizontal Size:                   63 cm
  Horizontal Frequency:                   135 - 135 kHz
  Vertical Frequency:                     40 - 60 Hz
  Maximum Pixel Clock:                    600 MHz
 [Advanced parameters]
  Input Signal:                           Digital
  Color Bit Depth:                        10 Bits per Primary Color
  Digital Video Interface Standard Supported: DisplayPort
  Gamma Factor:                           2.20
 [DPMS Modes]
  Standby:                                Not Supported
  Suspend:                                Not Supported
  Active Off:                             Supported
  Standard Colour Space (sRGB) Default:   Not Supported
  Preferred Timing Mode:                  Supported
  Default GTF (Continuous Frequency):     Supported
  DFP 1.x Compatible:                     Yes
 [Supported Video Modes]
  1152 x 864                              75 Hz
  1280 x 800                              60 Hz
  1280 x 720                              60 Hz
  1280 x 1024                             60 Hz
  1600 x 900                              60 Hz
  1680 x 1050                             60 Hz
  1440 x 900                              60 Hz
  3840 x 2160                             632 x 360 mm, Pixel Clock 533.25 MHz

Drives --------------------------------------------------------------------


(S)ATA/ATAPI Drives -------------------------------------------------------


NVMe Drives ---------------------------------------------------------------


PM961 NVMe SAMSUNG 512GB --------------------------------------------------

 [General Information]
  Drive Controller:                       NVMe (PCIe 4x 8.0 GT/s)
  Host Controller:                        Samsung Electronics SSD 960 NVMe PCIe SSD Controller
  Drive Model:                            PM961 NVMe SAMSUNG 512GB
  Drive Serial Number:                          S33YNB0J501455
  Drive Firmware Revision:                CXY74D1Q
  NVMe Version Supported:                 v1.2
  Drive Capacity:                         488,386 MBytes (512 GB)
  Drive Capacity [MB]:                    488386
 [Capabilities]
  Volatile Write Cache:                   Present
  Compare Command:                        Supported
  Write Uncorrectable Command:            Supported
  Dataset Management:                     Supported
  Write Zeroes:                           Supported
  Save field set to a non-zero value:     Supported
  Reservations:                           Not Supported
  Timestamp:                              Not Supported
  Autonomous Power State Transitions:     Supported
 [Self-Monitoring, Analysis and Reporting Technology (S.M.A.R.T.)]
  Available Space Below Threshold:        OK
  Temperature Exceeded Critical Threshold: OK
  Device Reliablity Degraded:             OK
  Media In Read Only Mode:                OK
  Volatile Memory Backup Device Failed:   OK
  Drive Temperature:                      38 °C
  Warning Temperature Threshold:          68 °C
  Critical Temperature Threshold:         71 °C
  Time Above Warning Temperature Threshold: 0 minutes
  Time Above Critical Temperature Threshold: 0 minutes
  Spare Capacity Available:               100%
  Device Health:                          95%
  Power Cycles:                           3082
  Power On Hours:                         5564 hours
  Unsafe Shutdowns:                       130
  Media Errors:                           0
  Total Host Reads:                       31153 GBytes
  Total Host Writes:                      33526 GBytes

WDC WDS960G2G0C-00AJM0 ----------------------------------------------------

 [General Information]
  Drive Controller:                       IDE <-> USB
  Host Controller:                        Realtek Semiconductor, PID=F192
  Drive Channel:                          Primary, Slave
  Drive Model:                            WDC WDS960G2G0C-00AJM0
  Drive Firmware Revision:                231800WD
  Drive Serial Number:                    21284M800322
  Drive Capacity:                         Unknown
 [Drive Geometry]
  Number of Cylinders:                    0
  Number of Heads:                        0
  Sectors Per Track:                      0
  Bytes Per Sector:                       10
  Bytes Per Track:                        10688
  Logical Sector Size:                    512 Bytes
  Cache Buffer Size:                      N/A
 [Transfer Modes]
  Max. PIO Transfer Mode:                 0
  Multiword DMA Mode:                     Total: -, Active: -
  Singleword DMA Mode:                    Total: -, Active: -
  Ultra-DMA Mode:                         N/A
  Max. DMA Transfer Rate:                 N/A
  Max. PIO with IORDY Transfer Rate:      N/A
  Max. PIO w/o IORDY Transfer Rate:       N/A
  Transfer Width:                         16-bit
  Native Command Queuing:                 Not Supported
  TRIM Command:                           Not Supported
 [Device flags]
  Fixed Drive:                            Not Present
  Removable Drive:                        Not Present
  Magnetic Storage:                       Present
  LBA Mode:                               Not Supported
  DMA Mode:                               Not Supported
  IORDY:                                  Not Supported
  IORDY Disableable:                      Not Supported
 [Features]
  Write Cache:                            Not Present, Inactive
  S.M.A.R.T. Feature:                     Not Present, Inactive
  Security Feature:                       Not Present, Inactive
  Removable Media Feature:                Not Present, Disabled
  Power Management:                       Not Present, Inactive
  Advanced Power Management:              Not Present, Inactive
  Packet Interface:                       Not Present, Disabled
  Look-Ahead Buffer:                      Not Present, Inactive
  Host Protected Area:                    Not Present, Disabled
  Power-Up In Standby:                    Not Supported, Inactive
  Automatic Acoustic Management:          Not Supported, Inactive
  48-bit LBA:                             Not Supported, Inactive
  Host-Initiated Link Power Management (HIPM): Not Supported
  Device-Initiated Link Power Management (DIPM): Not Supported
  In-Order Data Delivery:                 Not Supported
  Hardware Feature Control:               Not Supported
  Software Settings Preservation:         Not Supported
  NCQ Autosense:                          Not Supported
  Link Power State Device Sleep:          Not Supported
  Hybrid Information Feature:             Not Supported
  Rebuild Assist:                         Not Supported
  Power Disable:                          Not Supported
  All Write Cache Non-Volatile:           Not Supported
  Extended Number of User Addressable Sectors: Not Supported
  CFast Specification:                    Not Supported
  NCQ Priority Information:               Not Supported
  Host Automatic Partial to Slumber Transitions: Not Supported
  Device Automatic Partial to Slumber Transitions: Not Supported
  NCQ Streaming:                          Not Supported
  NCQ Queue Management Command:           Not Supported
  DevSleep to Reduced Power State:        Not Supported
  Out Of Band Management Interface:       Not Supported
 [Security]
  Security Feature:                       Not Supported
  Security Status:                        Disabled
  Security Locked:                        Disabled
  Security Frozen:                        Disabled
  Enhanced Security Erase:                Not Supported
  Sanitize Feature:                       Not Supported
  Sanitize Device - Crypto Scramble:      Not Supported
  Sanitize Device - Overwrite:            Not Supported
  Sanitize Device - Block Erase:          Not Supported
  Sanitize Device - Antifreeze Lock:      Not Supported
  Device Encrypts All User Data:          Not Supported
  Trusted Computing:                      Not Supported
 [Self-Monitoring, Analysis and Reporting Technology (S.M.A.R.T.)]

Sabrent -------------------------------------------------------------------

 [General information]
  Drive Model:                            Sabrent
  Drive Firmware Revision:                1.00
  Device Type:                            Disk drive
  Drive Capacity:                         915,715 MBytes (960 GB)
  Drive Capacity [MB]:                    915715

MSFT XVDD -----------------------------------------------------------------

 [General information]
  Drive Model:                            MSFT XVDD
  Drive Firmware Revision:                1.0
  Device Type:                            Disk drive

Audio ---------------------------------------------------------------------


Intel Wellsburg PCH - High Definition Audio Controller [B1] ---------------

  Audio Adapter:                          Intel Wellsburg PCH - High Definition Audio Controller [B1]
  Audio Controller Hardware ID:           PCI\VEN_8086&DEV_8D20&SUBSYS_72708086&REV_05
  High Definition Audio Codec:            RealTek ALC662
  Audio Codec Hardware ID:                HDAUDIO\FUNC_01&VEN_10EC&DEV_0662&SUBSYS_10EC0662&REV_1003
 [Driver Information]
  Driver Manufacturer:                    Microsoft
  Driver Description:                     High Definition Audio Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            04-Jun-2021
  DeviceInstanceId                        HDAUDIO\FUNC_01&VEN_10EC&DEV_0662&SUBSYS_10EC0662&REV_1003\4&278B75BB&0&0001

ATI/AMD Navi1x - High Definition Audio Controller -------------------------

  Audio Adapter:                          ATI/AMD Navi1x - High Definition Audio Controller
  Audio Controller Hardware ID:           PCI\VEN_1002&DEV_AB38&SUBSYS_AB381002&REV_00
  High Definition Audio Codec:            ATi RADEON HDMI
  Audio Codec Hardware ID:                HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00AA0100&REV_1007
 [Driver Information]
  Driver Manufacturer:                    Advanced Micro Devices
  Driver Description:                     AMD High Definition Audio Device
  Driver Provider:                        Advanced Micro Devices
  Driver Version:                         10.0.1.23
  Driver Date:                            26-Jul-2021
  DeviceInstanceId                        HDAUDIO\FUNC_01&VEN_1002&DEV_AA01&SUBSYS_00AA0100&REV_1007\7&39F4490F&0&0001

Network -------------------------------------------------------------------


RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC -------------

 [General information]
  Network Card:                           RealTek Semiconductor RTL8168/8111 PCI-E Gigabit Ethernet NIC
  Vendor Description:                     Realtek PCIe GbE Family Controller
  MAC Address:                            2A-17-4C-07-01-C1
 [Capabilities]
  Maximum Link Speed:                     1000 Mbps
  Transmit Buffer Size:                   193792 Bytes
  Receive Buffer Size:                    775168 Bytes
  Hardware ID:                            PCI\VEN_10EC&DEV_8168&SUBSYS_012310EC&REV_09
 [Driver Information]
  Driver Manufacturer:                    Realtek
  Driver Description:                     Realtek PCIe GbE Family Controller
  Driver Provider:                        Microsoft
  Driver Version:                         9.1.411.2015
  Driver Date:                            10-Apr-2015
  DeviceInstanceId                        PCI\VEN_10EC&DEV_8168&SUBSYS_012310EC&REV_09\78000000684CE00000
  Location Paths                          PCIROOT(0)#PCI(1C07)#PCI(0000)

Ports ---------------------------------------------------------------------


Serial Ports --------------------------------------------------------------


USB -----------------------------------------------------------------------


Standard Enhanced PCI to USB Host Controller ------------------------------


Root Hub ------------------------------------------------------------------


[Port1] : Intel Integrated Rate Matching Hub ------------------------------

 [Device Information]
  Device Manufacturer:                    Intel
  Product Name:                           Intel Integrated Rate Matching Hub
  Serial Number:                          
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_8087&PID_8002
 [Driver Information]
  Driver Manufacturer:                    (Generic USB Hub)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_8087&PID_8002\5&12B5DBAE&0&1
  Location Paths                          PCIROOT(0)#PCI(1D00)#USBROOT(0)#USB(1)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : No Device Connected ---------------------------------------------


[Port7] : No Device Connected ---------------------------------------------


[Port8] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


Standard Enhanced PCI to USB Host Controller ------------------------------


Root Hub ------------------------------------------------------------------


[Port1] : Intel Integrated Rate Matching Hub ------------------------------

 [Device Information]
  Device Manufacturer:                    Intel
  Product Name:                           Intel Integrated Rate Matching Hub
  Serial Number:                          
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_8087&PID_800A
 [Driver Information]
  Driver Manufacturer:                    (Generic USB Hub)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_8087&PID_800A\5&117D1CCD&0&1
  Location Paths                          PCIROOT(0)#PCI(1A00)#USBROOT(0)#USB(1)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


Intel(R) USB 3.0 eXtensible Host Controller - 1.0 (Microsoft) -------------


Root Hub ------------------------------------------------------------------


[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port5] : No Device Connected ---------------------------------------------


[Port6] : Realtek Semiconductor 4-Port USB 3 Hub --------------------------

 [Device Information]
  Device Manufacturer:                    Generic
  Product Name:                           4-Port USB 2.0 Hub
  Serial Number:                          N/A
  USB Version Supported:                  3.00 (Connected to a USB 2.00 Port)
  USB Device Speed:                       USB 2.0 High-speed
  Driver Description:                     Generic USB Hub
  Hardware ID:                            USB\VID_0BDA&PID_5411
 [Driver Information]
  Driver Manufacturer:                    (Standard USB HUBs)
  Driver Description:                     Generic USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.65
  Driver Date:                            02-Jul-2021
  DeviceInstanceId                        USB\VID_0BDA&PID_5411\5&1932DDEF&0&6
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(6)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : Holtek Microelectronics, PID=FC02 -------------------------------

 [Device Information]
  Device Manufacturer:                    OBINS
  Product Name:                           OBINS
AnnePro2
  Serial Number:                          00000000000000000000000000000000
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 1.1 Full-speed
  Driver Description:                     USB Composite Device
  Hardware ID:                            USB\VID_04D9&PID_A293
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     USB Composite Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_04D9&PID_A293\00000000000000000000000000000000
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(6)#USB(4)

[Port7] : No Device Connected ---------------------------------------------


[Port8] : No Device Connected ---------------------------------------------


[Port9] : No Device Connected ---------------------------------------------


[Port10] : No Device Connected --------------------------------------------


[Port11] : No Device Connected --------------------------------------------


[Port12] : No Device Connected --------------------------------------------


[Port13] : No Device Connected --------------------------------------------


[Port14] : Logitech Cordless Mouse ----------------------------------------

 [Device Information]
  Device Manufacturer:                    Logitech
  Product Name:                           USB Receiver
  Serial Number:                          N/A
  USB Version Supported:                  2.00
  USB Device Speed:                       USB 1.1 Full-speed
  Driver Description:                     USB Composite Device
  Hardware ID:                            USB\VID_046D&PID_C52F
 [Driver Information]
  Driver Manufacturer:                    (Standard USB Host Controller)
  Driver Description:                     USB Composite Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.1
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_046D&PID_C52F\5&1932DDEF&0&14
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(14)

[Port15] : No Device Connected --------------------------------------------


[Port16] : No Device Connected --------------------------------------------


[Port17] : SanDisk Ultra Flair --------------------------------------------

 [Device Information]
  Device Manufacturer:                    SanDisk
  Product Name:                           Ultra USB 3.0
  Serial Number:                          04014b313b1ab4c951b133dec56456ad315c981acc6dff524ddfdfc4abf95501586a00000000000000000000cc104d700015081891558107b3a7208b
  USB Version Supported:                  3.00
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     USB Mass Storage Device
  Hardware ID:                            USB\VID_0781&PID_5591
 [Driver Information]
  Driver Manufacturer:                    Compatible USB storage device
  Driver Description:                     USB Mass Storage Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.653
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_0781&PID_5591\04014B313B1AB4C951B133DEC56456AD315C981ACC6DFF524DDFDFC4ABF95501586A00000000000000000000CC104D700015081891558107B3A7208B
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(17)

[Port18] : Realtek Semiconductor, PID=F192 --------------------------------

 [Device Information]
  Device Manufacturer:                    Sabrent
  Product Name:                           Sabrent
  Serial Number:                          012345678930
  USB Version Supported:                  3.20
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     USB Attached SCSI (UAS) Mass Storage Device
  Hardware ID:                            USB\VID_0BDA&PID_9210
 [Driver Information]
  Driver Manufacturer:                    USB Attached SCSI (UAS) Compatible Device
  Driver Description:                     USB Attached SCSI (UAS) Mass Storage Device
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.653
  Driver Date:                            20-Jun-2006
  DeviceInstanceId                        USB\VID_0BDA&PID_9210\MSFT30012345678930
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(18)

[Port19] : Realtek Semiconductor 4-Port USB 3 Hub -------------------------

 [Device Information]
  Device Manufacturer:                    Realtek Semiconductor
  Product Name:                           Realtek Semiconductor 4-Port USB 3 Hub
  Serial Number:                          -
  USB Version Supported:                  3.00
  USB Device Speed:                       USB 3.0 SuperSpeed
  Driver Description:                     Generic SuperSpeed USB Hub
  Hardware ID:                            USB\VID_0BDA&PID_0411
 [Driver Information]
  Driver Manufacturer:                    (Standard USB HUBs)
  Driver Description:                     Generic SuperSpeed USB Hub
  Driver Provider:                        Microsoft
  Driver Version:                         10.0.22000.65
  Driver Date:                            02-Jul-2021
  DeviceInstanceId                        USB\VID_0BDA&PID_0411\5&1932DDEF&0&19
  Location Paths                          PCIROOT(0)#PCI(1400)#USBROOT(0)#USB(19)

[Port1] : No Device Connected ---------------------------------------------


[Port2] : No Device Connected ---------------------------------------------


[Port3] : No Device Connected ---------------------------------------------


[Port4] : No Device Connected ---------------------------------------------


[Port20] : No Device Connected --------------------------------------------


[Port21] : No Device Connected --------------------------------------------

